	RASTPCX.EXE - raster to .PCX conversion for OrCAD	pd 970726
	-------------------------------------------------
	
	- Change output driver to RAST150.DRV or RAST200.DRV
	- PRINTALL YOURSCH.SCH X - this creates the raster file X.
	- RASTPCX X X
	- DEL X
	- Don't forget to change output driver back to normal printer driver.
	
	Output files are named X001.PCX, X002.PCX, etc.
	
	You may have to crop the .PCX files. One way to do this is to load
	them into Windows 95 Paint, change the size in Image/Attributes
	and save the file (as .BMP). You can then insert the bitmap into
	Word etc.
	
	pd 020419	Recompiled using current Borland Pascal unit,
			this should avoid crashes.
