PrintPlotOutputDescription( bidi_pln.pfg ) Units( inches )
      DriverOptions( GerberFormat34, ClearAPXOnBeginAll )
  LargestAperture( 2.0000 )

PageName( 1 ) Output( bidi_c1.ger ) Device( Gerber-274X )

  Scale( 1.000000 )
  DimensionScale( 1.000000 )
  OffsetX( 0.0000 )
  OffsetY( 0.0000 )
       PageOptions( MirrorY )
   Layer( ComponentCopper )
      SolderGuard( OnlyObjectSolderGuard )
      Include( Pads, Nets, Vias, TestPoints, LayerMarkers, Circles, Outlines )
      Include( Text, AlignmentTargets )
      Options( CopperPour, MirrorText )

PageName( 2 ) Output( bidi_c2.ger ) Device( Gerber-274X )

  Scale( 1.000000 )
  DimensionScale( 1.000000 )
  OffsetX( 0.0000 )
  OffsetY( 0.0000 )
        PageOptions( MirrorY )
  Layer( SolderCopper )
      SolderGuard( OnlyObjectSolderGuard )
      Include( Pads, Nets, Vias, TestPoints, LayerMarkers, Circles, Outlines )
      Include( Text, AlignmentTargets )
      Options( CopperPour )

PageName( 3 ) Output( bidi_dr.ger ) Device( Gerber-274X )

  Scale( 1.000000 )
  DimensionScale( 1.000000 )
  OffsetX( 0.0000 )
  OffsetY( 0.0000 )
      PageOptions( MirrorY )
    DrillHolesBetweenLayers( SolderCopper,ComponentCopper )
    DrillLegend( Right )
    DrillTargets( Symbols )
      SolderGuard( OnlyObjectSolderGuard )
      Include( Pads, Vias, AlignmentTargets, Outlines, Holes )
    

