This disk set contains the OrCAD Schematic Design Tools 386+ update.

INSTALLING SCHEMATIC DESIGN TOOLS 386+ UPDATE

1. Insert the first update disk in your computer's floppy disk drive.

2. Change drive to the floppy drive where you placed the first update disk.
   For example, if the drive containing the update disk is A, then at the DOS
   prompt type "A:" and press the enter or return key.
   
3. Now at the DOS prompt type "INSTALL" and press enter or return key.

From this point on, INSTALL will prompt you to enter any additional
information it needs to install the SDT 386+ update.
