;*******************************************************************************
; Copyright 2001-2005 Broadcom Corporation.
;
; INF for 32-bit Windows 2K, Windows XP and Windows server 2003
;
; InfVersion   8.22.1.0.C
;
;*******************************************************************************


[Version]
Signature   = "$Windows NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
CatalogFile = b57win32.cat
Compatible  = 1
Provider    = %BRCM%
DriverVer   = 04/20/2005,8.22.1.0

[Manufacturer]
%BRCM% = Broadcom, NTx86.5.1, NTamd64

[Broadcom]
%OEM1_DEV5% = OEM1_DEV5.Inst, PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5% = OEM1_DEV5.Inst, PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV5% = OEM1_DEV5.Inst, PCI\VEN_14e4&DEV_165D&SUBSYS_019c1028
%OEM1_DEV6% = OEM1_DEV6.Inst, PCI\VEN_14e4&DEV_1653&SUBSYS_86531028

%BCM5700%   = BCM5700.Inst,   PCI\VEN_14e4&DEV_1644
%BCM5701%   = BCM5701.Inst,   PCI\VEN_14e4&DEV_1645
%BCM5702%   = BCM5702.Inst,   PCI\VEN_14e4&DEV_1646
%BCM5702%   = BCM5702.Inst,   PCI\VEN_14e4&DEV_16A6
%BCM5702%   = BCM5702A3.Inst, PCI\VEN_14e4&DEV_16C6
%BCM5703%   = BCM5703.Inst,   PCI\VEN_14e4&DEV_1647
%BCM5703%   = BCM5703.Inst,   PCI\VEN_14e4&DEV_16A7
%BCM5703%   = BCM5703A3.Inst, PCI\VEN_14e4&DEV_16C7
%BCM5704%   = BCM5704.Inst,   PCI\VEN_14e4&DEV_1648
%BCM5705%   = BCM5705.Inst,   PCI\VEN_14e4&DEV_1653
%BCM5705M%  = BCM5705M.Inst,  PCI\VEN_14e4&DEV_165D
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e
%BCM5705F%  = BCM5705F.Inst,  PCI\VEN_14e4&DEV_166e
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_05721014
%BCM5705M%  = BCM5705MA2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_0727152d

%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_167C&REV_00
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_167D&REV_00

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1658
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1676
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_167C
%BCM5750A1%   = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_167D



; BB  0x167D AX Revs
%BCM5750%   = BCM5750.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01

; BB  0x167D BX, CX, XX  Revs
%BCM5750A1%   = BCM5750MIBM.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_05771014

; BB  0x167E AX Revs
%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01

; BB  0x167E BX, CX, XX  Revs
%BCM5750A1F%   = BCM5750FIBM.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014


%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014



%BCM5750A1F%   = BCM5750A1F.Inst,   PCI\VEN_14e4&DEV_167E

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_10961734

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1

%BCM5750A1%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_00631025

%BCM5901%   = BCM5901.Inst,   PCI\VEN_14e4&DEV_170D
%BCM5901%   = BCM5901.Inst,   PCI\VEN_14e4&DEV_170e
%BCM5782%   = BCM5782.Inst,   PCI\VEN_14e4&DEV_1696
%BCM5788%   = BCM5788.Inst,   PCI\VEN_14e4&DEV_169c
%BCM5789%   = BCM5789.Inst,   PCI\VEN_14e4&DEV_169d

%BCM5788%   = BCM5788.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d

%BCM5788%   = BCM5788F1.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_123c10cf
%BCM5788%   = BCM5788F1.Inst,   PCI\VEN_14e4&DEV_169c&SUBSYS_12f710cf
%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_127910cf
%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5750A1%   = BCM5750A1F3.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5789%   = BCM5789F1.Inst,   PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5750A1%   = BCM5750A1F3M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1%   = BCM5750A1F3M.Inst,  PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1%   = BCM5750A1F3M.Inst,   PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1%   = BCM5750A1F3.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1%   = BCM5750A1F3.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033

%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%  = BCM5705MA2F2.Inst,PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033

%BCM5700FB% = BCM5700FB.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5700FA% = BCM5700FA.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5701FA% = BCM5701FA.Inst, PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5703S%  = BCM5703S.Inst,  PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%  = BCM5703S.Inst,  PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703SW% = BCM5703SW.Inst, PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5703S%  = BCM5703SA3.Inst,PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5704S%  = BCM5704S.Inst,  PCI\VEN_14e4&DEV_16A8
%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW% = BCM5704SW.Inst, PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5750A1%   = BCM5750A1.Inst, PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014

%3C996T%    = 3C996T.Inst,    PCI\VEN_14e4&DEV_1644&SUBSYS_100010B7
%3C996SX%   = 3C996SX.Inst,   PCI\VEN_14e4&DEV_1645&SUBSYS_100410B7
%3C996BT%   = 3C996BT.Inst,   PCI\VEN_14e4&DEV_1645&SUBSYS_100610B7
%3C1000T%   = 3C1000T.Inst,   PCI\VEN_14e4&DEV_1645&SUBSYS_100710B7
%3C940BR01% = 3C940BR01.Inst, PCI\VEN_14e4&DEV_1645&SUBSYS_100810B7
%3C998T%    = 3C998T.Inst,    PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C998SX%   = 3C998SX.Inst,   PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C999T%    = 3C999T.Inst,    PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%3C1000BT%  = 3C1000BT.Inst,  PCI\VEN_14e4&DEV_16A6&SUBSYS_110010B7
%3C1000BT%  = 3C1000BTA3.Inst,PCI\VEN_14e4&DEV_16C6&SUBSYS_110010B7

%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%   = BCM5705A2.Inst, PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014

%OEM1_DEV1% = OEM1_DEV1.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_102814e4
%OEM1_DEV1% = OEM1_DEV1.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_00d11028
%OEM1_DEV2% = OEM1_DEV2.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_01091028
%OEM1_DEV3% = OEM1_DEV3.Inst, PCI\VEN_14e4&DEV_1644&SUBSYS_010A1028
%OEM1_DEV4% = OEM1_DEV4.Inst, PCI\VEN_14e4&DEV_16A6&SUBSYS_81261028

%OEM1_DEV7% = OEM1_DEV4.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV7% = OEM1_DEV4.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV7% = OEM1_DEV4.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV7% = OEM1_DEV4.Inst, PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028

%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01791028

%OEM1_DEV6%     = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01801028
%OEM1_DEV6%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_01851028
%OEM1_DEV6%   = BCM5750A1.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_01841028

%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028

%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.Inst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028

%BCM5750A1STSP%   = BCM5750A1STSP.Inst,   PCI\VEN_14e4&DEV_1659&SUBSYS_3260103C

%BCM5705M%  = BCM5705MA2.Inst,          PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5901%   = BCM5901.Inst,             PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%   = BCM5901.Inst,             PCI\VEN_14e4&DEV_170E&SUBSYS_05451014
%BCM5750A1%   = BCM5750A1.Inst,             PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014

; 12X12
%BCM5750A1%    = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_16F7
%BCM5750A1%    = BCM5750A1M.Inst,   PCI\VEN_14e4&DEV_16FD
%BCM5789%       = BCM5789.Inst,         PCI\VEN_14e4&DEV_16DD

%BCM5750A1%    = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_16F7&SUBSYS_02f61014
%BCM5750A1%    = BCM5750A1.Inst,     PCI\VEN_14e4&DEV_16F7&SUBSYS_02f91014



[Broadcom.NTx86.5.1]
%OEM1_DEV5% = OEM1_DEV5XP.XpInst, PCI\VEN_14e4&DEV_165D&SUBSYS_865d1028
%OEM1_DEV5% = OEM1_DEV5XP.XpInst, PCI\VEN_14e4&DEV_165D&SUBSYS_20031028
%OEM1_DEV6% = OEM1_DEV6XP.XpInst, PCI\VEN_14e4&DEV_1653&SUBSYS_86531028


%BCM5700%   = BCM5700.XpInst,   PCI\VEN_14e4&DEV_1644
%BCM5700%   = BCM5700CX.XpInst, PCI\VEN_14e4&DEV_1644&REV_21
%BCM5700%   = BCM5700CX.XpInst, PCI\VEN_14e4&DEV_1644&REV_22
%BCM5701%   = BCM5701.XpInst,   PCI\VEN_14e4&DEV_1645
%BCM5702%   = BCM5702.XpInst,   PCI\VEN_14e4&DEV_1646
%BCM5702%   = BCM5702.XpInst,   PCI\VEN_14e4&DEV_16A6
%BCM5702%   = BCM5702.XpInst,   PCI\VEN_14e4&DEV_16C6
%BCM5703%   = BCM5703.XpInst,   PCI\VEN_14e4&DEV_16A7
%BCM5703%   = BCM5703.XpInst,   PCI\VEN_14e4&DEV_1647
%BCM5703%   = BCM5703.XpInst,   PCI\VEN_14e4&DEV_16C7
%BCM5704%   = BCM5704.XpInst,   PCI\VEN_14e4&DEV_1648
%BCM5705%   = BCM5705.XpInst,   PCI\VEN_14e4&DEV_1653
%BCM5705M%  = BCM5705M.XpInst,  PCI\VEN_14e4&DEV_165D
%BCM5705%   = BCM5705A2.XpInst, PCI\VEN_14e4&DEV_1654
%BCM5705M%  = BCM5705MA2.XpInst,PCI\VEN_14e4&DEV_165E
%BCM5705M%  = BCM5705MA2.XpInst,PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5705M%  = BCM5705MA2.XpInst,PCI\VEN_14e4&DEV_165E&SUBSYS_0727152d

%BCM5750%   = BCM5750.XpInst,   PCI\VEN_14e4&DEV_1658&REV_00
%BCM5750%   = BCM5750.XpInst,   PCI\VEN_14e4&DEV_1659&REV_00
%BCM5750%   = BCM5750.XpInst,   PCI\VEN_14e4&DEV_1676&REV_00
%BCM5750%   = BCM5750.XpInst,   PCI\VEN_14e4&DEV_1677&REV_00
%BCM5750%   = BCM5750.XpInst,   PCI\VEN_14e4&DEV_167C&REV_00

%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1658
%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1659
%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1676
%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677
%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_167C
%BCM5750A1%   = BCM5750A1M.XpInst,   PCI\VEN_14e4&DEV_167D


; BB  0x167D AX Revs
%BCM5750%   = BCM5750.XpInst,   PCI\VEN_14e4&DEV_167D&SUBSYS_05771014&REV_01

; BB  0x167D BX, CX, XX  Revs
%BCM5750A1%   = BCM5750MIBM.XpInst,   PCI\VEN_14e4&DEV_167D&SUBSYS_05771014

; BB  0x167E AX Revs
%BCM5750A1F%   = BCM5750A1F.XpInst,   PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014&REV_01

; BB  0x167E BX, CX, XX  Revs
%BCM5750A1F%   = BCM5750FIBM.XpInst,   PCI\VEN_14e4&DEV_167E&SUBSYS_057D1014


%BCM5750A1F%   = BCM5750A1F.XpInst,   PCI\VEN_14e4&DEV_167E&SUBSYS_02F71014



%BCM5750A1F%   = BCM5750A1F.XpInst,   PCI\VEN_14e4&DEV_167E

%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_105D1734
%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1659&SUBSYS_10611734
%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_10961734

%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_267610f1

%BCM5750A1%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_00631025

%BCM5750A1%   = BCM5750A1SPECIAL.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_81AA104D

%BCM5901%   = BCM5901.XpInst,   PCI\VEN_14e4&DEV_170D
%BCM5901%   = BCM5901.XpInst,   PCI\VEN_14e4&DEV_170E
%BCM5782%   = BCM5705A2.XpInst, PCI\VEN_14e4&DEV_1696
%BCM5788%   = BCM5788.XpInst,   PCI\VEN_14e4&DEV_169C
%BCM5789%   = BCM5789.XpInst,   PCI\VEN_14e4&DEV_169d
%BCM5705F%  = BCM5705F.XpInst,  PCI\VEN_14e4&DEV_166e

%BCM5788%   = BCM5788.XpInst,   PCI\VEN_14e4&DEV_169c&SUBSYS_c016144d

%BCM5788%   = BCM5788F1.XpInst,   PCI\VEN_14e4&DEV_169C&SUBSYS_123c10cf
%BCM5788%   = BCM5788F1.XpInst,   PCI\VEN_14e4&DEV_169C&SUBSYS_12f710cf
%BCM5705M%  = BCM5705MA2F2.XpInst,PCI\VEN_14e4&DEV_165E&SUBSYS_127910cf
%BCM5705M%  = BCM5705MA2F2.XpInst,PCI\VEN_14e4&DEV_1654&SUBSYS_12f810cf
%BCM5750A1% = BCM5750A1F3.XpInst, PCI\VEN_14e4&DEV_1677&SUBSYS_128810cf
%BCM5789%   = BCM5789F1.XpInst,   PCI\VEN_14e4&DEV_169d&SUBSYS_12ff10cf
%BCM5750A1% = BCM5750A1F3M.XpInst,PCI\VEN_14e4&DEV_167D&SUBSYS_130010cf
%BCM5750A1% = BCM5750A1F3M.XpInst,  PCI\VEN_14e4&DEV_167D&SUBSYS_131510cf
%BCM5750A1% = BCM5750A1F3M.XpInst,PCI\VEN_14e4&DEV_167D&SUBSYS_82c31033
%BCM5750A1% = BCM5750A1F3.XpInst,PCI\VEN_14e4&DEV_1677&SUBSYS_82d31033
%BCM5750A1% = BCM5750A1F3.XpInst,PCI\VEN_14e4&DEV_1677&SUBSYS_82ee1033

%BCM5705M%  = BCM5705MA2F2.XpInst,PCI\VEN_14e4&DEV_1654&SUBSYS_82581033
%BCM5705M%  = BCM5705MA2F2.XpInst,PCI\VEN_14e4&DEV_1654&SUBSYS_825c1033
%BCM5705M%  = BCM5705MA2F2.XpInst,PCI\VEN_14e4&DEV_165e&SUBSYS_82c51033

%BCM5700FB% = BCM5700FB.XpInst, PCI\VEN_14e4&DEV_1644&SUBSYS_000214e4
%BCM5700FA% = BCM5700FA.XpInst, PCI\VEN_14e4&DEV_1644&SUBSYS_000314e4
%BCM5701FA% = BCM5701FA.XpInst, PCI\VEN_14e4&DEV_1645&SUBSYS_000714e4
%BCM5703S%  = BCM5703S.XpInst,  PCI\VEN_14e4&DEV_16A7&SUBSYS_000a14e4
%BCM5703S%  = BCM5703S.XpInst,  PCI\VEN_14e4&DEV_1647&SUBSYS_000a14e4
%BCM5703S%  = BCM5703S.XpInst,  PCI\VEN_14e4&DEV_16C7&SUBSYS_000a14e4
%BCM5703SW% = BCM5703SW.XPInst, PCI\VEN_14e4&DEV_16A7&SUBSYS_02811014
%BCM5704S%  = BCM5704S.XPInst,  PCI\VEN_14e4&DEV_16A8
%BCM5704SW% = BCM5704SW.XPInst, PCI\VEN_14e4&DEV_16A8&SUBSYS_029c1014
%BCM5704SW% = BCM5704SW.XPInst, PCI\VEN_14e4&DEV_16A8&SUBSYS_02a81014
%BCM5704SW% = BCM5704SW.XPInst, PCI\VEN_14e4&DEV_16A8&SUBSYS_02e81014
%BCM5704SW% = BCM5704SW.XPInst, PCI\VEN_14e4&DEV_16A8&SUBSYS_02e91014
%BCM5704SW% = BCM5704SW.XPInst, PCI\VEN_14e4&DEV_16A8&SUBSYS_03011014
%BCM5750A1%   = BCM5750A1.XpInst, PCI\VEN_14e4&DEV_1677&SUBSYS_02F71014


%3C996T%    = 3C996T.XpInst,    PCI\VEN_14e4&DEV_1644&SUBSYS_100010B7
%3C996SX%   = 3C996SX.XpInst,   PCI\VEN_14e4&DEV_1645&SUBSYS_100410B7
%3C996BT%   = 3C996BT.XpInst,   PCI\VEN_14e4&DEV_1645&SUBSYS_100610B7
%3C1000T%   = 3C1000T.XpInst,   PCI\VEN_14e4&DEV_1645&SUBSYS_100710B7
%3C940BR01% = 3C940BR01.XpInst, PCI\VEN_14e4&DEV_1645&SUBSYS_100810B7
%3C998T%    = 3C998T.XpInst,    PCI\VEN_14e4&DEV_1648&SUBSYS_200010B7
%3C998SX%   = 3C998SX.XpInst,   PCI\VEN_14e4&DEV_16A8&SUBSYS_200110B7
%3C999T%    = 3C999T.XpInst,    PCI\VEN_14e4&DEV_1648&SUBSYS_300010B7
%3C1000BT%  = 3C1000BT.XpInst,  PCI\VEN_14e4&DEV_16A6&SUBSYS_110010B7
%3C1000BT%  = 3C1000BT.XpInst,  PCI\VEN_14e4&DEV_16C6&SUBSYS_110010B7

%BCM5705%   = BCM5705A2.XpInst, PCI\VEN_14e4&DEV_1654&SUBSYS_02b51014
%BCM5705%   = BCM5705A2.XpInst, PCI\VEN_14e4&DEV_1654&SUBSYS_02b61014
%BCM5705%   = BCM5705A2.XpInst, PCI\VEN_14e4&DEV_1654&SUBSYS_02D81014
%BCM5705%   = BCM5705A2.XpInst, PCI\VEN_14e4&DEV_1654&SUBSYS_02D91014
%BCM5705%   = BCM5705A2.XpInst, PCI\VEN_14e4&DEV_1654&SUBSYS_02F81014

%OEM1_DEV1% = OEM1_DEV1.XpInst, PCI\VEN_14e4&DEV_1644&SUBSYS_102814e4
%OEM1_DEV1% = OEM1_DEV1.XpInst, PCI\VEN_14e4&DEV_1644&SUBSYS_00d11028
%OEM1_DEV2% = OEM1_DEV2.XpInst, PCI\VEN_14e4&DEV_1644&SUBSYS_01091028
%OEM1_DEV3% = OEM1_DEV3.XpInst, PCI\VEN_14e4&DEV_1644&SUBSYS_010A1028
%OEM1_DEV4% = OEM1_DEV4XP.XpInst, PCI\VEN_14e4&DEV_16A6&SUBSYS_81261028

%OEM1_DEV4% = OEM1_DEV4XP.XpInst, PCI\VEN_14e4&DEV_165e&SUBSYS_01711028
%OEM1_DEV4% = OEM1_DEV4XP.XpInst, PCI\VEN_14e4&DEV_165e&SUBSYS_015a1028
%OEM1_DEV4% = OEM1_DEV4XP.XpInst, PCI\VEN_14e4&DEV_165e&SUBSYS_017c1028
%OEM1_DEV4% = OEM1_DEV4XP.XpInst, PCI\VEN_14e4&DEV_165e&SUBSYS_01AA1028

%BCM5750A1DDT%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01751028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01761028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01771028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01781028
%BCM5750A1DDT%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01791028

%BCM5750A1DSF%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01801028
%BCM5750A1DSSF%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1659&SUBSYS_01851028
%BCM5750A1DSSF%   = BCM5750A1.XpInst,   PCI\VEN_14e4&DEV_1659&SUBSYS_01841028

%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01AD1028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01A81028
%BCM5750A1DMOBILE%     = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01A91028


%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01821028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01861028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01871028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01881028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_018f1028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01a01028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_01a31028
%BCM5750A1DMOBILE%   = BCM5750A1DMOBILE.XpInst,   PCI\VEN_14e4&DEV_1677&SUBSYS_019c1028

%BCM5750A1STSP%   = BCM5750A1STSP.XpInst,   PCI\VEN_14e4&DEV_1659&SUBSYS_3260103c

%BCM5705M%  = BCM5705MA2.XpInst,        PCI\VEN_14e4&DEV_165E&SUBSYS_05721014
%BCM5901%   = BCM5901.XpInst,           PCI\VEN_14e4&DEV_170D&SUBSYS_05451014
%BCM5901%   = BCM5901.XpInst,           PCI\VEN_14e4&DEV_170E&SUBSYS_05451014
%BCM5750A1%   = BCM5750A1.XpInst,           PCI\VEN_14e4&DEV_1659&SUBSYS_02FE1014


; 12X12
%BCM5750A1%    = BCM5750A1.XpInst,     PCI\VEN_14e4&DEV_16F7
%BCM5750A1%    = BCM5750A1M.XpInst,   PCI\VEN_14e4&DEV_16FD
%BCM5789%       = BCM5789.XpInst,         PCI\VEN_14e4&DEV_16DD

%BCM5750A1%    = BCM5750A1.XpInst,     PCI\VEN_14e4&DEV_16F7&SUBSYS_02f61014
%BCM5750A1%    = BCM5750A1.XpInst,     PCI\VEN_14e4&DEV_16F7&SUBSYS_02f91014

[Broadcom.NTamd64]
        
[ControlFlags]
ExcludeFromSelect = *

;*******************************************************************************
; 32-bit Windows 2K Install sections.
;*******************************************************************************

[BCM5700.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700.AddService, NtEventLog

[BCM5700.AddService]
DisplayName    = %BCM5700%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5701.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5701.Inst.NT.Services]
AddService = b57w2k, 2, BCM5701.AddService, NtEventLog

[BCM5701.AddService]
DisplayName    = %BCM5701%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5702.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5702.Inst.NT.Services]
AddService = b57w2k, 2, BCM5702.AddService, NtEventLog

[BCM5702.AddService]
DisplayName    = %BCM5702%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5702A3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5702A3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5702A3.AddService, NtEventLog

[BCM5702A3.AddService]
DisplayName    = %BCM5702%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703.AddService, NtEventLog

[BCM5703.AddService]
DisplayName    = %BCM5703%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703A3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703A3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703A3.AddService, NtEventLog

[BCM5703A3.AddService]
DisplayName    = %BCM5703%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5704.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704.Inst.NT.Services]
AddService = b57w2k, 2, BCM5704.AddService, NtEventLog

[BCM5704.AddService]
DisplayName    = %BCM5704%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705.AddService, NtEventLog

[BCM5705.AddService]
DisplayName    = %BCM5705%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705A2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705A2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705A2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705A2.AddService, NtEventLog

[BCM5705A2.AddService]
DisplayName    = %BCM5705%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5782.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5782.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5782.Inst.NT.Services]
AddService = b57w2k, 2, BCM5782.AddService, NtEventLog

[BCM5782.AddService]
DisplayName    = %BCM5782%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5788.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5788.Inst.NT.Services]
AddService = b57w2k, 2, BCM5788.AddService, NtEventLog

[BCM5788.AddService]
DisplayName    = %BCM5788%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5788F1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5788.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5788F1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5788F1.AddService, NtEventLog

[BCM5788F1.AddService]
DisplayName    = %BCM5788%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5705M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705M.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705M.AddService, NtEventLog

[BCM5705M.AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705MA2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705MA2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705MA2.AddService, NtEventLog

[BCM5705MA2.AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5705MA2F2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5705MA2.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705MA2F2.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705MA2F2.AddService, NtEventLog

[BCM5705MA2F2.AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5901.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5901.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5901.Inst.NT.Services]
AddService = b57w2k, 2, BCM5901.AddService, NtEventLog

[BCM5901.AddService]
DisplayName    = %BCM5901%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5705F.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5705F.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5705F.Inst.NT.Services]
AddService = b57w2k, 2, BCM5705F.AddService, NtEventLog

[BCM5705F.AddService]
DisplayName    = %BCM5705F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5700FB.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700FB.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700FB.AddService, NtEventLog

[BCM5700FB.AddService]
DisplayName    = %BCM5700FB%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5700FA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5700FA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5700FA.AddService, NtEventLog

[BCM5700FA.AddService]
DisplayName    = %BCM5700FA%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5701FA.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5701FA.Inst.NT.Services]
AddService = b57w2k, 2, BCM5701FA.AddService, NtEventLog

[BCM5701FA.AddService]
DisplayName    = %BCM5701FA%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5703S.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703S.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703S.AddService, NtEventLog

[BCM5703S.AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703SA3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703SA3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703SA3.AddService, NtEventLog

[BCM5703SA3.AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5703SW.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5703.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5703SW.Inst.NT.Services]
AddService = b57w2k, 2, BCM5703SW.AddService, NtEventLog

[BCM5703SW.AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5704S.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704S.Inst.NT.Services]
AddService = b57w2k, 2, BCM5704S.AddService, NtEventLog

[BCM5704S.AddService]
DisplayName    = %BCM5704S%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5704SW.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5704.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsWOLTbi
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5704SW.Inst.NT.Services]
AddService = b57w2k, 2, BCM5704SW.AddService, NtEventLog

[BCM5704SW.AddService]
DisplayName    = %BCM5704SW%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5750.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShasta, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750.AddService, NtEventLog

[BCM5750.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5789.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5789.Inst.NT.Services]
AddService = b57w2k, 2, BCM5789.AddService, NtEventLog

[BCM5789.AddService]
DisplayName    = %BCM5789%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5789F1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5789F1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5789F1.AddService, NtEventLog

[BCM5789F1.AddService]
DisplayName    = %BCM5789%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5750A1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1.AddService, NtEventLog

[BCM5750A1.AddService]
DisplayName    = %BCM5750A1%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5750A1STSP.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1STSP.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1STSP.AddService, NtEventLog

[BCM5750A1STSP.AddService]
DisplayName    = %BCM5750A1STSP%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5750A1M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1M.AddService, NtEventLog

[BCM5750A1M.AddService]
DisplayName    = %BCM5750A1%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5750MIBM.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsM,  ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750MIBM.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750MIBM.AddService, NtEventLog

[BCM5750MIBM.AddService]
DisplayName    = %BCM5750A1%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5750B0M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750B0M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750B0M.AddService, NtEventLog

[BCM5750B0M.AddService]
DisplayName    = %BCM5750B0%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5750B0MF.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLShastaFull, ParamsWireSpeed, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750B0MF.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750B0MF.AddService, NtEventLog

[BCM5750B0MF.AddService]
DisplayName    = %BCM5750B0F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5750A1F.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLShastaFull, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1MF.AddService, NtEventLog

[BCM5750A1MF.AddService]
DisplayName    = %BCM5750A1F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5750FIBM.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsC100, ParamsWOLShastaFull, ParamsWireSpeed, ParamsWOLLink
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750FIBM.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750FIBM.AddService, NtEventLog

[BCM5750FIBM.AddService]
DisplayName    = %BCM5750A1F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS



[BCM5750A1DMOBILE.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = NtAddReg, BCM5750.Params, ParamsNt8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLShastaFullMOBILE, DMobile.Params
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1DMOBILE.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1DMOBILE.AddService, NtEventLog

[BCM5750A1DMOBILE.AddService]
DisplayName    = %BCM5750A1DMOBILE%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[BCM5750A1F3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1F3.AddService, NtEventLog

[BCM5750A1F3.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[BCM5750A1F3M.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = NtAddReg, BCM5750.Params, ParamsNt, ParamsNt8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.NtSys
BusType         = 5

[BCM5750A1F3M.Inst.NT.Services]
AddService = b57w2k, 2, BCM5750A1F3M.AddService, NtEventLog

[BCM5750A1F3M.AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[3C996T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C996T.Inst.NT.Services]
AddService = b57w2k, 2, 3C996T.AddService, NtEventLog

[3C996T.AddService]
DisplayName    = %3C996T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C996SX.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C996SX.Inst.NT.Services]
AddService = b57w2k, 2, 3C996SX.AddService, NtEventLog

[3C996SX.AddService]
DisplayName    = %3C996SX%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C996BT.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C996BT.Inst.NT.Services]
AddService = b57w2k, 2, 3C996BT.AddService, NtEventLog

[3C996BT.AddService]
DisplayName    = %3C996BT%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C1000T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C1000T.Inst.NT.Services]
AddService = b57w2k, 2, 3C1000T.AddService, NtEventLog

[3C1000T.AddService]
DisplayName    = %3C1000T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C940BR01.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5701.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C940BR01.Inst.NT.Services]
AddService = b57w2k, 2, 3C940BR01.AddService, NtEventLog

[3C940BR01.AddService]
DisplayName    = %3C940BR01%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C998T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C998T.Inst.NT.Services]
AddService = b57w2k, 2, 3C998T.AddService, NtEventLog

[3C998T.AddService]
DisplayName    = %3C998T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C998SX.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C998SX.Inst.NT.Services]
AddService = b57w2k, 2, 3C998SX.AddService, NtEventLog

[3C998SX.AddService]
DisplayName    = %3C998SX%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C999T.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C999T.Inst.NT.Services]
AddService = b57w2k, 2, 3C999T.AddService, NtEventLog

[3C999T.AddService]
DisplayName    = %3C999T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C1000BT.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C1000BT.Inst.NT.Services]
AddService = b57w2k, 2, 3C1000BT.AddService, NtEventLog

[3C1000BT.AddService]
DisplayName    = %3C1000BT%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[3C1000BTA3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsWireSpeed
CopyFiles       = CopyFile.NtSys
BusType         = 5

[3C1000BTA3.Inst.NT.Services]
AddService = b57w2k, 2, 3C1000BTA3.AddService, NtEventLog

[3C1000BTA3.AddService]
DisplayName    = %3C1000BT%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[OEM1_DEV1.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV1.Inst.NT.Services]
AddService = b57w2k, 2, OEM1_DEV1.AddService, NtEventLog

[OEM1_DEV1.AddService]
DisplayName    = %OEM1_DEV1%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[OEM1_DEV2.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV2.Inst.NT.Services]
AddService = b57w2k, 2, OEM1_DEV2.AddService, NtEventLog

[OEM1_DEV2.AddService]
DisplayName    = %OEM1_DEV2%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[OEM1_DEV3.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = NtAddReg, BCM5700.Params, ParamsNt, ParamsNt8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV3.Inst.NT.Services]
AddService = b57w2k, 2, OEM1_DEV3.AddService, NtEventLog

[OEM1_DEV3.AddService]
DisplayName    = %OEM1_DEV3%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS


[OEM1_DEV4.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5702.Params, OEM1_DEV4.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV4.Inst.NT.Services]
AddService = b57w2k, 2, OEM1_DEV4.AddService, NtEventLog

[OEM1_DEV4.AddService]
DisplayName    = %OEM1_DEV4%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[OEM1_DEV5.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5705M.Params, OEM1_DEV5.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV5.Inst.NT.Services]
AddService = b57w2k, 2, OEM1_DEV5.AddService, NtEventLog

[OEM1_DEV5.AddService]
DisplayName    = %OEM1_DEV5%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

[OEM1_DEV6.Inst.NT]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = NtAddReg, BCM5705.Params, OEM1_DEV6.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.NtSys
BusType         = 5

[OEM1_DEV6.Inst.NT.Services]
AddService = b57w2k, 2, OEM1_DEV6.AddService, NtEventLog

[OEM1_DEV6.AddService]
DisplayName    = %OEM1_DEV6%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57w2k.sys
LoadOrderGroup = NDIS

;*******************************************************************************
; 32-bit Windows XP Install sections.
;*******************************************************************************

[BCM5700.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700.Xp32AddService, Xp32EventLog

[BCM5700.Xp32AddService]
DisplayName    = %BCM5700%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5700CX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700CX.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700CX.Xp32AddService, Xp32EventLog

[BCM5700CX.Xp32AddService]
DisplayName    = %BCM5700%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5701.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5701.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5701.Xp32AddService, Xp32EventLog

[BCM5701.Xp32AddService]
DisplayName    = %BCM5701%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5702.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5702.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5702.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5702.Xp32AddService, Xp32EventLog

[BCM5702.Xp32AddService]
DisplayName    = %BCM5702%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5703.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5703.Xp32AddService, Xp32EventLog

[BCM5703.Xp32AddService]
DisplayName    = %BCM5703%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5704.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5704.Xp32AddService, Xp32EventLog

[BCM5704.Xp32AddService]
DisplayName    = %BCM5704%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5705.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705.Xp32AddService, Xp32EventLog

[BCM5705.Xp32AddService]
DisplayName    = %BCM5705%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5750.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShasta, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750.Xp32AddService, Xp32EventLog

[BCM5750.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1.Xp32AddService, Xp32EventLog

[BCM5750A1.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1STSP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1STSP.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1STSP.Xp32AddService, Xp32EventLog

[BCM5750A1STSP.Xp32AddService]
DisplayName    = %BCM5750A1STSP%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5789.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5789.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5789.Xp32AddService, Xp32EventLog

[BCM5789.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5789F1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5789F1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5789F1.Xp32AddService, Xp32EventLog

[BCM5789F1.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5750B0M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750B0M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750B0M.Xp32AddService, Xp32EventLog

[BCM5750B0M.Xp32AddService]
DisplayName    = %BCM5750B0%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750B0MF.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750B0MF.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750B0MF.Xp32AddService, Xp32EventLog

[BCM5750B0MF.Xp32AddService]
DisplayName    = %BCM5750B0F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5750A1SPECIAL.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xSPECIAL, ParamsCSPECIAL, ParamsWOLShastaFull, ParamsWireSpeedSPECIAL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1SPECIAL.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1SPECIAL.Xp32AddService, Xp32EventLog

[BCM5750A1SPECIAL.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1M.Xp32AddService, Xp32EventLog

[BCM5750A1M.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750MIBM.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd, ParamsM, ParamsWOLLink
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750MIBM.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750MIBM.Xp32AddService, Xp32EventLog

[BCM5750MIBM.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750FIBM.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLShastaFull, ParamsWireSpeed, ParamsWOLLink, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750FIBM.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750FIBM.Xp32AddService, Xp32EventLog

[BCM5750FIBM.Xp32AddService]
DisplayName    = %BCM5750A1F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1F.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1F.Xp32AddService, Xp32EventLog

[BCM5750A1F.Xp32AddService]
DisplayName    = %BCM5750A1F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5750A1DMOBILE.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNT8021p, ParamsNtW9xMOBILE, ParamsC, ParamsWOLShastaFullMOBILE, DMobileXP.Params
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1DMOBILE.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1DMOBILE.Xp32AddService, Xp32EventLog

[BCM5750A1DMOBILE.Xp32AddService]
DisplayName    = %BCM5750A1DDT%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1F3.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1F3.Xp32AddService, Xp32EventLog

[BCM5750A1F3.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5750A1F3M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
DelReg          = DelReg.ClockControl
AddReg          = Xp32AddReg, BCM5750.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ , ParamsC, ParamsWOLShastaFull, ParamsWireSpeed, ParamsLgSnd, ParamsLogOptions, ParamsM
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5750A1F3M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5750A1F3M.Xp32AddService, Xp32EventLog

[BCM5750A1F3M.Xp32AddService]
DisplayName    = %BCM5750%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5705M.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705M.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsWireSpeed, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705M.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705M.Xp32AddService, Xp32EventLog

[BCM5705M.Xp32AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5705F.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705F.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705F.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705F.Xp32AddService, Xp32EventLog

[BCM5705F.Xp32AddService]
DisplayName    = %BCM5705F%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5705A2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705A2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705A2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705A2.Xp32AddService, Xp32EventLog

[BCM5705A2.Xp32AddService]
DisplayName    = %BCM5705%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5705MA2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705MA2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705MA2.Xp32AddService, Xp32EventLog

[BCM5705MA2.Xp32AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5705MA2F2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5705MA2.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5705MA2F2.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5705MA2F2.Xp32AddService, Xp32EventLog

[BCM5705MA2F2.Xp32AddService]
DisplayName    = %BCM5705M%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5901.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.LgSnd
AddReg          = Xp32AddReg, BCM5901.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC100, ParamsWOL
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5901.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5901.Xp32AddService, Xp32EventLog

[BCM5901.Xp32AddService]
DisplayName    = %BCM5901%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5788.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsC, ParamsWOL, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5788.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5788.Xp32AddService, Xp32EventLog

[BCM5788.Xp32AddService]
DisplayName    = %BCM5788%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5788F1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5788.Params, ParamsNt, ParamsNT8021p, ParamsNtW9xFJ, ParamsC, ParamsWOL, ParamsLgSnd, ParamsLogOptions
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5788F1.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5788F1.Xp32AddService, Xp32EventLog

[BCM5788F1.Xp32AddService]
DisplayName    = %BCM5788%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[BCM5700FB.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700FB.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700FB.Xp32AddService, Xp32EventLog

[BCM5700FB.Xp32AddService]
DisplayName    = %BCM5700FB%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5700FA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5700FA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5700FA.Xp32AddService, Xp32EventLog

[BCM5700FA.Xp32AddService]
DisplayName    = %BCM5700FA%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5701FA.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5701FA.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5701FA.Xp32AddService, Xp32EventLog

[BCM5701FA.Xp32AddService]
DisplayName    = %BCM5701FA%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[BCM5703S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5703S.Xp32AddService, Xp32EventLog

[BCM5703S.Xp32AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5703SW.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5703.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5703SW.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5703SW.Xp32AddService, Xp32EventLog

[BCM5703SW.Xp32AddService]
DisplayName    = %BCM5703S%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5704S.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704S.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5704S.Xp32AddService, Xp32EventLog

[BCM5704S.Xp32AddService]
DisplayName    = %BCM5704S%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[BCM5704SW.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5704.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd, ParamsWOLTbi
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[BCM5704SW.XpInst.NTx86.Services]
AddService = b57w2k, 2, BCM5704SW.Xp32AddService, Xp32EventLog

[BCM5704SW.Xp32AddService]
DisplayName    = %BCM5704SW%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C996T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C996T.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C996T.Xp32AddService, Xp32EventLog

[3C996T.Xp32AddService]
DisplayName    = %3C996T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C996SX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.RequestedMediaType, DelReg.Wol, DelReg.WireSpeed
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsLgSnd
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C996SX.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C996SX.Xp32AddService, Xp32EventLog

[3C996SX.Xp32AddService]
DisplayName    = %3C996SX%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C996BT.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C996BT.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C996BT.Xp32AddService, Xp32EventLog

[3C996BT.Xp32AddService]
DisplayName    = %3C996BT%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C998T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C998T.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C998T.Xp32AddService, Xp32EventLog

[3C998T.Xp32AddService]
DisplayName    = %3C998T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C998SX.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C998SX.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C998SX.Xp32AddService, Xp32EventLog

[3C998SX.Xp32AddService]
DisplayName    = %3C998SX%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C999T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C999T.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C999T.Xp32AddService, Xp32EventLog

[3C999T.Xp32AddService]
DisplayName    = %3C999T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[3C1000T.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C1000T.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C1000T.Xp32AddService, Xp32EventLog

[3C1000T.Xp32AddService]
DisplayName    = %3C1000T%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C940BR01.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5701.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C940BR01.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C940BR01.Xp32AddService, Xp32EventLog

[3C940BR01.Xp32AddService]
DisplayName    = %3C940BR01%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[3C1000BT.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5702.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOL, ParamsLgSnd, ParamsWireSpeed
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[3C1000BT.XpInst.NTx86.Services]
AddService = b57w2k, 2, 3C1000BT.Xp32AddService, Xp32EventLog

[3C1000BT.Xp32AddService]
DisplayName    = %3C1000BT%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[OEM1_DEV1.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV1.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV1.Xp32AddService, Xp32EventLog

[OEM1_DEV1.Xp32AddService]
DisplayName    = %OEM1_DEV1%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[OEM1_DEV2.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV2.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV2.Xp32AddService, Xp32EventLog

[OEM1_DEV2.Xp32AddService]
DisplayName    = %OEM1_DEV2%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[OEM1_DEV3.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.WolS
AddReg          = Xp32AddReg, BCM5700.Params, ParamsNt, ParamsNT8021p, ParamsNtW9x, ParamsJumbo, ParamsC, ParamsWOLNS, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV3.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV3.Xp32AddService, Xp32EventLog

[OEM1_DEV3.Xp32AddService]
DisplayName    = %OEM1_DEV3%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[OEM1_DEV4.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5702.Params, OEM1_DEV4.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV4.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV4.Xp32AddService, Xp32EventLog

[OEM1_DEV4.Xp32AddService]
DisplayName    = %OEM1_DEV4%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[OEM1_DEV5.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5705M.Params, OEM1_DEV5.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV5.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV5.Xp32AddService, Xp32EventLog

[OEM1_DEV5.Xp32AddService]
DisplayName    = %OEM1_DEV5%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS

[OEM1_DEV6.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
AddReg          = Xp32AddReg, BCM5705.Params, OEM1_DEV6.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV6.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV6.Xp32AddService, Xp32EventLog

[OEM1_DEV6.Xp32AddService]
DisplayName    = %OEM1_DEV6%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[OEM1_DEV4XP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5702.Params, OEM1_DEV4.Params, ParamsNT8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV4XP.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV4XP.Xp32AddService, Xp32EventLog

[OEM1_DEV4XP.Xp32AddService]
DisplayName    = %OEM1_DEV4%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



[OEM1_DEV5XP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705M.Params, OEM1_DEV5.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV5XP.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV5XP.Xp32AddService, Xp32EventLog

[OEM1_DEV5XP.Xp32AddService]
DisplayName    = %OEM1_DEV5%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS


[OEM1_DEV6XP.XpInst.NTx86]
Characteristics = 0x84 ; NCF_HAS_UI | NCF_PHYSICAL
DelReg          = DelReg.Jumbo
AddReg          = Xp32AddReg, BCM5705M.Params, OEM1_DEV6.Params, ParamsNt8021p, ParamsC, ParamsWOLNS, ParamsFlow, DriverInfo
CopyFiles       = CopyFile.XpSys32
BusType         = 5

[OEM1_DEV6XP.XpInst.NTx86.Services]
AddService = b57w2k, 2, OEM1_DEV6XP.Xp32AddService, Xp32EventLog

[OEM1_DEV6XP.Xp32AddService]
DisplayName    = %OEM1_DEV6%
ServiceType    = 1 
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\b57xp32.sys
LoadOrderGroup = NDIS



;*******************************************************************************
; Windows 2k common sections.
;*******************************************************************************

[NtAddReg]
HKR, Ndi,            Service,    0, "b57w2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[NtEventLog]
AddReg = NtAddEventLogReg

[NtAddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57w2k.sys"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; 32-bit Windows Xp common sections.
;*******************************************************************************

[Xp32AddReg]
HKR, Ndi,            Service,    0, "b57w2k"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[Xp32EventLog]
AddReg = Xp32AddEventLogReg

[Xp32AddEventLogReg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\drivers\b57xp32.sys"
HKR, , TypesSupported  , 0x00010001, 7



;*******************************************************************************
; Registry parameters.
;*******************************************************************************

[BCM5700.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "360"
HKR, , TxCoalescingTicks,        0, "360"
HKR, , RxMaxCoalescedFrames,     0, "15"
HKR, , TxMaxCoalescedFrames,     0, "75"


[BCM5701.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5702.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5703.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"


[BCM5704.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705M.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705F.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705A2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5705MA2.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5750.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5901.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[BCM5788.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[OEM1_DEV4.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV5.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[OEM1_DEV6.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"

[DMobile.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WireSpeed,                0, "1"


[OEM1_DEV4XP.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"
HKR, , LargeSendOffload,         0, "1"

[OEM1_DEV5XP.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"
HKR, , LargeSendOffload,         0, "1"

[OEM1_DEV6XP.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WolSpeed,                 0, "0"
HKR, , WireSpeed,                0, "1"
HKR, , LargeSendOffload,         0, "1"

[DMobileXP.Params]
HKR, , TaskOffloadCap,           0, "21"
HKR, , RxMtu,                    0, "1514"
HKR, , WireSpeed,                0, "1"
HKR, , LargeSendOffload,         0, "1"


[BCM5782.Params]
HKR, , TxPacketDescCnt,          0, "200"
HKR, , RxStdDescCnt,             0, "200"
HKR, , RxCoalescingTicks,        0, "10"
HKR, , TxCoalescingTicks,        0, "30"
HKR, , RxMaxCoalescedFrames,     0, "5"
HKR, , TxMaxCoalescedFrames,     0, "200"

[ParamsNt]
HKR, Ndi\Params\TaskOffloadCap,      ParamDesc, , %TaskOffload%
HKR, Ndi\Params\TaskOffloadCap,      default,   , "63"
HKR, Ndi\Params\TaskOffloadCap,      type,      , "enum"
HKR, Ndi\Params\TaskOffloadCap\enum, 0,         , %TaskOffload_None%
HKR, Ndi\Params\TaskOffloadCap\enum, 42,        , %TaskOffload_Rx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 21,        , %TaskOffload_Tx_Chksum%
HKR, Ndi\Params\TaskOffloadCap\enum, 63,        , %TaskOffload_Rx_Tx_Chksum%

[ParamsNT8021p]
HKR, Ndi\Params\Enable8021p,      ParamDesc, , %QOS_8021p%
HKR, Ndi\Params\Enable8021p,      default,   , "0"
HKR, Ndi\Params\Enable8021p,      type,      , "enum"
HKR, Ndi\Params\Enable8021p\enum, 0,         , %QOS_8021p_Disable%
HKR, Ndi\Params\Enable8021p\enum, 1,         , %QOS_8021p_Enable%

[ParamsNtW9x]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"


[ParamsNtW9xFJ]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "0"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"



[ParamsNtW9xMOBILE]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%


[ParamsNtW9xSPECIAL]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

HKR, Ndi\params\NetworkAddress,        ParamDesc,  0, %NetworkAddress%
HKR, Ndi\params\NetworkAddress,        Default,    0, ""
HKR, Ndi\params\NetworkAddress,        type,       0, "edit"
HKR, NDI\params\NetworkAddress,        LimitText,  0, "12"
HKR, NDI\params\NetworkAddress,        UpperCase,  0, "1"
HKR, NDI\params\NetworkAddress,        optional,   0, "1"

[ParamsJumbo]
HKR, Ndi\Params\RxMtu, ParamDesc, , %JumboMtu%
HKR, Ndi\Params\RxMtu, default,   , "1500"
HKR, Ndi\Params\RxMtu, type,      , "dword"
HKR, Ndi\Params\RxMtu, min,       , "1500"
HKR, Ndi\Params\RxMtu, max,       , "9000"
HKR, Ndi\Params\RxMtu, step,      , "500"
HKR, Ndi\Params\RxMtu, base,      , "10"

[ParamsWireSpeed]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   0,         , %WireSpeed_Disable%
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%


[ParamsWOLLink]
HKR, Ndi\Params\WakeOnLink,        ParamDesc, , %WakeOnLink%
HKR, Ndi\Params\WakeOnLink,        default,   , "0"
HKR, Ndi\Params\WakeOnLink,        type,      , "enum"
HKR, Ndi\Params\WakeOnLink\enum,   0,         , %WakeOnLink_Disable%
HKR, Ndi\Params\WakeOnLink\enum,   1,         , %WakeOnLink_Enable%



[ParamsWireSpeedSPECIAL]
HKR, Ndi\Params\WireSpeed,        ParamDesc, , %WireSpeed%
HKR, Ndi\Params\WireSpeed,        default,   , "1"
HKR, Ndi\Params\WireSpeed,        type,      , "enum"
HKR, Ndi\Params\WireSpeed\enum,   1,         , %WireSpeed_Enable%

[ParamsLogOptions]
HKR, Ndi\Params\LogLevelInfo,        ParamDesc, , %LogLevelInfo%
HKR, Ndi\Params\LogLevelInfo,        default,   , "0"
HKR, Ndi\Params\LogLevelInfo,        type,      , "enum"
HKR, Ndi\Params\LogLevelInfo\enum,   0,         , %LogLevelInfo_Disable%
HKR, Ndi\Params\LogLevelInfo\enum,   1,         , %LogLevelInfo_Enable%
HKR, Ndi\Params\LogLevelWarn,        ParamDesc, , %LogLevelWarn%
HKR, Ndi\Params\LogLevelWarn,        default,   , "0"
HKR, Ndi\Params\LogLevelWarn,        type,      , "enum"
HKR, Ndi\Params\LogLevelWarn\enum,   0,         , %LogLevelWarn_Disable%
HKR, Ndi\Params\LogLevelWarn\enum,   1,         , %LogLevelWarn_Enable%


[ParamsC]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%

[ParamsCSPECIAL]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%

[ParamsC100]
HKR, Ndi\Params\RequestedMediaType,      ParamDesc, , %Speed_Duplex%
HKR, Ndi\Params\RequestedMediaType,      default,   , "0"
HKR, Ndi\Params\RequestedMediaType,      type,      , "enum"
HKR, Ndi\Params\RequestedMediaType\enum, 0,         , %Speed_Duplex_Auto%
HKR, Ndi\Params\RequestedMediaType\enum, 3,         , %Speed_Duplex_10Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 4,         , %Speed_Duplex_10Mb_Fd%
HKR, Ndi\Params\RequestedMediaType\enum, 5,         , %Speed_Duplex_100Mb_Hd%
HKR, Ndi\Params\RequestedMediaType\enum, 6,         , %Speed_Duplex_100Mb_Fd%


[ParamsWOL]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%

[ParamsWOLShasta]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
; HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
; HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
; HKR, Ndi\Params\WolSpeed\enum,  3,         , %WolSpeed_1000mb%

[ParamsWOLShastaFull]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

HKR, Ndi\Params\WolSpeed,       ParamDesc, , %WolSpeed%
HKR, Ndi\Params\WolSpeed,       default,   , "0"
HKR, Ndi\Params\WolSpeed,       type,      , "enum"
HKR, Ndi\Params\WolSpeed\enum,  0,         , %WolSpeed_Auto%
HKR, Ndi\Params\WolSpeed\enum,  1,         , %WolSpeed_10mb%
HKR, Ndi\Params\WolSpeed\enum,  2,         , %WolSpeed_100mb%
; HKR, Ndi\Params\WolSpeed\enum,  3,         , %WolSpeed_1000mb%


[ParamsWOLShastaFullMOBILE]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%


[ParamsM]
HKR, , ClockControl,          0, "1"

[ParamsWOLTbi]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "1"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, , TbiWol,                   0, "1"

[ParamsLgSnd]
HKR, Ndi\Params\LargeSendOffload,    ParamDesc, , %TaskOffload_LargeSend%
HKR, Ndi\Params\LargeSendOffload,    default,   , "1"
HKR, Ndi\Params\LargeSendOffload,      type,     , "enum"
HKR, Ndi\Params\LargeSendOffload\enum, 0,        , %TaskOffload_LargeSend_Disable%
HKR, Ndi\Params\LargeSendOffload\enum, 1,        , %TaskOffload_LargeSend_Enable%

[ParamsWOLNS]
HKR, Ndi\Params\WakeUpModeCap,       ParamDesc, , %WakeUpMode%
HKR, Ndi\Params\WakeUpModeCap,       default,   , "3"
HKR, Ndi\Params\WakeUpModeCap,       type,      , "enum"
HKR, Ndi\Params\WakeUpModeCap\enum,  0,         , %WakeUpMode_None%
HKR, Ndi\Params\WakeUpModeCap\enum,  1,         , %WakeUpMode_Magic%
HKR, Ndi\Params\WakeUpModeCap\enum,  2,         , %WakeUpMode_Pattern%
HKR, Ndi\Params\WakeUpModeCap\enum,  3,         , %WakeUpMode_Both%

[ParamsFlow]
HKR, Ndi\Params\FlowControlCap,      ParamDesc,  , %FlowControl%
HKR, Ndi\Params\FlowControlCap,      default,    , "2147483648"
HKR, Ndi\Params\FlowControlCap,      type,       , "enum"
HKR, Ndi\Params\FlowControlCap\enum, 0,          , %FlowControl_Disable%
HKR, Ndi\Params\FlowControlCap\enum, 1,          , %FlowControl_Rx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2,          , %FlowControl_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 3,          , %FlowControl_Rx_Tx_Pause%
HKR, Ndi\Params\FlowControlCap\enum, 2147483648, , %FlowControl_Auto%

;*******************************************************************************
; DriverInfo section.
;*******************************************************************************

[DriverInfo]
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Description,,%DriverDescription%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,CurrentVer,,%DriverOEMVersion%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,Ver_%DriverOEMVersion%,,%DriverVersionID%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,BaseDriverFileName,,%BaseDriverFileName%
HKLM,Software\InstalledOptions\%DriverOEM%\%DriverFamily%\%DriverMfgr%\%DriverProduct%,BaseDriverFileVersion,,%BaseDriverFileVersion%



;*******************************************************************************
; Keys to remove.
;*******************************************************************************

[DelReg.RequestedMediaType]
HKR, Ndi\Params\RequestedMediaType

[DelReg.Wol]
HKR, Ndi\Params\WolSpeed
HKR, Ndi\Params\WakeUpModeCap

[DelReg.WolS]
HKR, Ndi\Params\WolSpeed

[DelReg.Jumbo]
HKR, Ndi\Params\RxMtu

[DelReg.LgSnd]
HKR, Ndi\Params\LargeSendOffload

[DelReg.WireSpeed]
HKR, Ndi\Params\WireSpeed

[DelReg.ClockControl]
HKR, ,ClockControl

;*******************************************************************************
; Destination directories
;*******************************************************************************

[DestinationDirs]
DefaultDestDir   = 11
CopyFile.XpSys32 = 12
CopyFile.NtSys  = 12

[SourceDisksNames]
1 = %DISK_DESC%,,,

[SourceDisksFiles]
b57xp32.sys = 1
b57w2k.sys = 1

[CopyFile.XpSys32]
b57xp32.sys,,,1

[CopyFile.NtSys]
b57w2k.sys,,,1



;*******************************************************************************
; Localizable strings
;*******************************************************************************

[Strings]
BRCM                = "Broadcom"
DISK_DESC           = "Broadcom NetXtreme Installation Media"

BCM5700             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5701             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5702             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5703             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705M            = "Broadcom NetXtreme Gigabit Ethernet"
BCM5705F            = "Broadcom 570x 10/100 Integrated Controller"
BCM5750             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750A1F          = "Broadcom NetXtreme Fast Ethernet"

BCM5750A1STSP    = "Embedded Broadcom NetXtreme 5721 PCI-E Gigabit NIC"

BCM5750B0           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5750B0F          = "Broadcom NetXtreme Fast Ethernet"

BCM5901             = "Broadcom NetXtreme Fast Ethernet"
BCM5782             = "Broadcom NetXtreme Gigabit Ethernet"
BCM5788             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5789             = "Broadcom NetLink (TM) Gigabit Ethernet"
BCM5700FB           = "Broadcom NetXtreme Gigabit Fiber"
BCM5700FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5701FA           = "Broadcom NetXtreme Gigabit Fiber"
BCM5703S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5703SW           = "Broadcom NetXtreme Gigabit Ethernet"
BCM5704S            = "Broadcom NetXtreme Gigabit Fiber"
BCM5704SW           = "Broadcom NetXtreme Gigabit Ethernet"

3C996T              = "3Com 3C996 10/100/1000 Server NIC"
3C996SX             = "3Com 3C996 Gigabit Fiber-SX Server NIC"
3C996BT             = "3Com 3C996B Gigabit Server NIC"
3C1000T             = "3Com 3C1000 Gigabit NIC"
3C940BR01           = "3Com 3C940 Gigabit LOM"
3C998T              = "3Com Dual Port 10/100/1000 PCI-X Server NIC"
3C998SX             = "3Com Dual Port 1000-SX PCI-X Server NIC"
3C999T              = "3Com Quad Port 10/100/1000 PCI-X Server NIC"
3C1000BT            = "3Com 10/100/1000 PCI"

OEM1_DEV1           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV2           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV3           = "Broadcom NetXtreme Gigabit Ethernet"
OEM1_DEV4           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV5           = "Broadcom 570x Gigabit Integrated Controller"
OEM1_DEV6           = "Broadcom NetXtreme Gigabit Ethernet"

BCM5750A1DSF      = "Broadcom NetXtreme 5751 Gigabit Controller"
BCM5750A1DSSF    = "Broadcom NetXtreme 5721 Gigabit Controller"
BCM5750A1DDT      = "Broadcom NetXtreme 57xx Gigabit Controller"
BCM5750A1DMOBILE =  "Broadcom NetXtreme 57xx Gigabit Controller"

OEM1_DEV7           = "Broadcom 570x Gigabit Integrated Controller"

; These items will be set by IHV...
DriverMfgr            = "Broadcom"                  ; IHV name
DriverVersionID       = "5.00"                      ; The IHV driver version
BaseDriverFileVersion = "8.22"
BaseDriverFileName    = "b57xp32.sys"               ; Key file for version

; These items will be set by IHV and updated by OEM
DriverOEM         = "Dell"      ; name of the OEM
DriverFamily      = "NIC"       ; device family (NIC, Storage, Video...)
DriverProduct     = "BCM5700"   ; Specific Name of device (chipset, for example)
DriverDescription = "Broadcom NetXtreme Gigabit Ethernet"  ; Description of device (product name, OS or system supported)
DriverOEMVersion  = "A00"       ; OEM-specified version


JumboMtu = "Jumbo Mtu"

FlowControl             = "Flow Control"
FlowControl_Disable     = "Disable"
FlowControl_Rx_Pause    = "Rx PAUSE"
FlowControl_Tx_Pause    = "Tx PAUSE"
FlowControl_Rx_Tx_Pause = "Rx/Tx PAUSE"
FlowControl_Auto        = "Auto"

Speed_Duplex          = "Speed & Duplex"
Speed_Duplex_Auto     = "Auto"
Speed_Duplex_10Mb_Hd  = "10 Mb Half"
Speed_Duplex_10Mb_Fd  = "10 Mb Full"
Speed_Duplex_100Mb_Hd = "100 Mb Half"
Speed_Duplex_100Mb_Fd = "100 Mb Full"
Speed_Duplex_1000Mb_Fd = "1000 Mb Full"

QOS_8021p         = "802.1p QOS"
QOS_8021p_Disable = "Disable"
QOS_8021p_Enable  = "Enable"

WireSpeed         = "Ethernet@WireSpeed"
WireSpeed_Disable = "Disable"
WireSpeed_Enable  = "Enable"

WakeOnLink         = "Wake On Link"
WakeOnLink_Disable = "Disable"
WakeOnLink_Enable  = "Enable"



TaskOffload              = "Checksum Offload"
TaskOffload_None         = "None"
TaskOffload_Rx_Chksum    = "Rx TCP/IP Checksum"
TaskOffload_Tx_Chksum    = "Tx TCP/IP Checksum"
TaskOffload_Rx_Tx_Chksum = "Tx/Rx TCP/IP Checksum"

TaskOffload_LargeSend           = "Large Send Offload"
TaskOffload_LargeSend_Disable   = "Disable"
TaskOffload_LargeSend_Enable    = "Enable"

WakeUpMode         = "Wake Up Capabilities"
WakeUpMode_None    = "None"
WakeUpMode_Magic   = "Magic Packet"
WakeUpMode_Pattern = "Wake Up Frame"
WakeUpMode_Both    = "Both"

WolSpeed       = "WOL Speed"
WolSpeed_Auto  = "Auto"
WolSpeed_10mb  = "10 Mb"
WolSpeed_100mb = "100 Mb"
WolSpeed_1000mb = "1000 Mb"

NetworkAddress           = "Locally Administered Address"


LogLevelInfo    = "Log Information Messages"
LogLevelWarn  = "Log Warning Messages"
LogLevelInfo_Disable  =  "Disable"
LogLevelInfo_Enable  =  "Enable"
LogLevelWarn_Disable  =  "Disable"
LogLevelWarn_Enable  =  "Enable"
