                           Broadcom Corporation
                           16215 Alton Parkway
                           Irvine, CA 92619-7013
			  
                               Release Notes                              
                               May 24, 2002


Windows NT Unattend Install Instructions
========================================


I. Introduction

    The unattend installation of Windows NT is achieved by setting the 
    options in the Unattend.txt file.


II. Setting up an Install Directory on the File Server
	
    The server must be setup with a distribution folder that holds the required 
    Windows NT files and which clients can reach when connecting via TCP/IP or IPX. 
    For examples in this bdrvcopy.txt use the network share C:\Image.

    To prepare the distribution folder:

	1.  Create a network share distribution folder, c:\Image
      	2.  Copy the \I386 folder from the Windows NT CD to C:\Image.
    	    Use Explorer, Winfile or XCOPY in order to maintain the same 
            directory structure as on the CD.
 	
        3.  Copy driver files from the Broadcom CD (found in \WinNT\Driver)
            into the shared directory C:\Image. 

	4.  Copy the Unattend folder from the Broadcom CD into the shared directory C:\Image.

	5.  Change directory to the Unattend folder on the Dos prompt

	6.  Run "BDRVCOPY.BAT ..\I386 nt" to create the driver install directory 
            structure and copy the driver files to it.

            This would make the following folders under the \I386 folder as follows:
	         \$oem$\drivers\BCM570X
		

III. Deployment Methods
	
    1. Make sure that you have a copy of a network bootable MS-DOS floppy that will 
       connect the client system to the C:\Image directory on the File Server.

    2. Map the network share c:\Image to Z: on the client system.

    3. CD to Z:\I386 directory and run the command:  

        winnt /s:z:\I386 /b /u:z:\I386\unattend.txt
       (where z: equals mapped drive)
