[preset00]
fRating=3.000000
fGammaAdj=1.000000
fDecay=1.000000
fVideoEchoZoom=0.999609
fVideoEchoAlpha=0.000000
nVideoEchoOrientation=1
nWaveMode=7
bAdditiveWaves=1
bWaveDots=0
bWaveThick=0
bModWaveAlphaByVolume=1
bMaximizeWaveColor=0
bTexWrap=0
bDarkenCenter=0
bRedBlueStereo=0
bBrighten=1
bDarken=0
bSolarize=0
bInvert=0
fWaveAlpha=4.099998
fWaveScale=1.285751
fWaveSmoothing=0.630000
fWaveParam=0.000000
fModWaveAlphaStart=0.710000
fModWaveAlphaEnd=1.300000
fWarpAnimSpeed=1.000000
fWarpScale=1.331000
fZoomExponent=1.000155
fShader=0.000000
zoom=1.009509
rot=0.000000
cx=0.500000
cy=0.500000
dx=0.000000
dy=0.000000
warp=0.010000
sx=1.000000
sy=1.000000
wave_r=0.650000
wave_g=0.650000
wave_b=0.650000
wave_x=0.500000
wave_y=0.500000
ob_size=0.500000
ob_r=0.010000
ob_g=0.000000
ob_b=0.000000
ob_a=0.000000
ib_size=0.260000
ib_r=0.250000
ib_g=0.250000
ib_b=0.250000
ib_a=0.000000
nMotionVectorsX=12.000000
nMotionVectorsY=9.000000
mv_dx=0.000000
mv_dy=0.000000
mv_l=0.900000
mv_r=1.000000
mv_g=1.000000
mv_b=1.000000
mv_a=0.000000
wavecode_0_enabled=0
wavecode_0_samples=512
wavecode_0_sep=0
wavecode_0_bSpectrum=1
wavecode_0_bUseDots=0
wavecode_0_bDrawThick=1
wavecode_0_bAdditive=0
wavecode_0_scaling=1.000000
wavecode_0_smoothing=0.000000
wavecode_0_r=0.000000
wavecode_0_g=0.000000
wavecode_0_b=0.000000
wavecode_0_a=1.000000
wave_0_per_point1=sp = sample*10;
wave_0_per_point2=ti = q1;
wave_0_per_point3=
wave_0_per_point4=ox = .25*sin(ti*.327 + sp*6.2832*3.12) + .5*sin(ti*.878 + sp*6.2832*8.68) + .25*sin(ti*.787 + sp*6.2832*7.85);
wave_0_per_point5=oy = .45*sin(ti*.877 + sp*6.2832*2.37) + .25*sin(ti*.482 + sp*6.2832*2.38) + .3*sin(ti*.129 + sp*6.2832*3.21);
wave_0_per_point6=oz = .35*sin(ti*.453 + sp*6.2832*8.97) + .15*sin(ti*.365 + sp*6.2832*5.13) + .5*sin(ti*.385 + sp*6.2832*5.46);
wave_0_per_point7=
wave_0_per_point8=ox = ox*6*q5;
wave_0_per_point9=oy = oy*6*q5;
wave_0_per_point10=oz = oz*6*q5;
wave_0_per_point11=
wave_0_per_point12=xang = q2;
wave_0_per_point13=yang = q3;
wave_0_per_point14=zang = q4;
wave_0_per_point15=
wave_0_per_point16=fov = .5;
wave_0_per_point17=
wave_0_per_point18=mx = ox*cos(yang) + oz*sin(yang);
wave_0_per_point19=mz = - ox*sin(yang) + oz*cos(yang);
wave_0_per_point20=ox = mx;
wave_0_per_point21=oz = mz;
wave_0_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_0_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_0_per_point24=ox = mx;
wave_0_per_point25=oy = my;
wave_0_per_point26=my = oy*cos(xang) - oz*sin(xang);
wave_0_per_point27=mz = oy*sin(xang) + oz*cos(xang);
wave_0_per_point28=oy = my;
wave_0_per_point29=oz = mz;
wave_0_per_point30=
wave_0_per_point31=oz = (oz - int(oz*.2)*5 - 5)*2;
wave_0_per_point32=x = ox*fov/oz + 0.5;
wave_0_per_point33=x = (x-.5)*0.75 + 0.5;
wave_0_per_point34=y = oy*fov/oz + 0.5;
wave_0_per_point35=
wave_0_per_point36=
wavecode_1_enabled=1
wavecode_1_samples=512
wavecode_1_sep=0
wavecode_1_bSpectrum=1
wavecode_1_bUseDots=1
wavecode_1_bDrawThick=1
wavecode_1_bAdditive=0
wavecode_1_scaling=1.000000
wavecode_1_smoothing=0.000000
wavecode_1_r=1.000000
wavecode_1_g=1.000000
wavecode_1_b=1.000000
wavecode_1_a=1.000000
wave_1_per_point1=sp = sample*10;
wave_1_per_point2=ti = q1;
wave_1_per_point3=
wave_1_per_point4=ox = .25*sin(ti*.654 + sp*6.2832*3.12) + .5*sin(ti*.378 + sp*6.2832*8.68) + .25*sin(ti*.537 + sp*6.2832*7.85);
wave_1_per_point5=oy = .45*sin(ti*.465 + sp*6.2832*2.37) + .25*sin(ti*.123 + sp*6.2832*2.38) + .3*sin(ti*.756 + sp*6.2832*3.21);
wave_1_per_point6=oz = .35*sin(ti*.758 + sp*6.2832*8.97) + .15*sin(ti*.187 + sp*6.2832*5.13) + .5*sin(ti*.548 + sp*6.2832*5.46);
wave_1_per_point7=
wave_1_per_point8=ox = ox*6*q5;
wave_1_per_point9=oy = oy*6*q5;
wave_1_per_point10=oz = oz*6*q5;
wave_1_per_point11=
wave_1_per_point12=xang = q2;
wave_1_per_point13=yang = q3;
wave_1_per_point14=zang = q4;
wave_1_per_point15=
wave_1_per_point16=fov = .5;
wave_1_per_point17=
wave_1_per_point18=mx = ox*cos(yang) + oz*sin(yang);
wave_1_per_point19=mz = - ox*sin(yang) + oz*cos(yang);
wave_1_per_point20=ox = mx;
wave_1_per_point21=oz = mz;
wave_1_per_point22=mx = ox*cos(zang) - oy*sin(zang);
wave_1_per_point23=my = ox*sin(zang) + oy*cos(zang);
wave_1_per_point24=ox = mx;
wave_1_per_point25=oy = my;
wave_1_per_point26=my = oy*cos(xang) - oz*sin(xang);
wave_1_per_point27=mz = oy*sin(xang) + oz*cos(xang);
wave_1_per_point28=oy = my;
wave_1_per_point29=oz = mz;
wave_1_per_point30=
wave_1_per_point31=oz = (oz - int(oz*.2)*5 - 5)*2;
wave_1_per_point32=x = ox*fov/oz + 0.5;
wave_1_per_point33=x = (x-.5)*0.75 + 0.5;
wave_1_per_point34=y = oy*fov/oz + 0.5;
wave_1_per_point35=
wave_1_per_point36=
wave_1_per_point37=
wave_1_per_point38=r=tan(x*6.28+3+q2);
wave_1_per_point39=r=min ( max(r*treb+0.5,0),1);
wave_1_per_point40=g=tan(y*6.28++32.1+q3);
wave_1_per_point41=g=min ( max(g*mid+0.5,0),1);
wave_1_per_point42=b=tan((x+y)*3.14+3+4.2+q4);
wave_1_per_point43=b=min ( max(b*bass+0.5,0),1);
wavecode_2_enabled=1
wavecode_2_samples=512
wavecode_2_sep=0
wavecode_2_bSpectrum=1
wavecode_2_bUseDots=0
wavecode_2_bDrawThick=1
wavecode_2_bAdditive=0
wavecode_2_scaling=1.000000
wavecode_2_smoothing=0.000000
wavecode_2_r=0.000000
wavecode_2_g=0.000000
wavecode_2_b=0.000000
wavecode_2_a=1.000000
wave_2_per_frame1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_2_per_frame2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_2_per_frame3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_2_per_frame4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_2_per_frame5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_2_per_frame6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_2_per_frame7=
wave_2_per_frame8=t1 = ra*6.2832;
wave_2_per_frame9=t2 = rb*6.2832;
wave_2_per_frame10=t3 = rc*6.2832;
wave_2_per_frame11=t4 = rd*6.2832;
wave_2_per_frame12=t5 = re*6.2832;
wave_2_per_frame13=t6 = rf*6.2832;
wave_2_per_frame14=
wave_2_per_frame15=rg = if(rg,rg,.1 + .8*rand(1001)*.001);
wave_2_per_frame16=rh = if(rh,rh,.1 + .8*rand(1001)*.001);
wave_2_per_frame17=
wave_2_per_frame18=t7 = rg;
wave_2_per_frame19=t8 = rh;
wave_2_per_frame20=
wave_2_per_frame21=
wave_2_per_frame22=tic = min(time-tir,.1);
wave_2_per_frame23=tir = time;
wave_2_per_frame24=ti = ti + tic*.5 + below(vr+vg+vb,.4)*tic*8;
wave_2_per_frame25=
wave_2_per_point1=ra = if(ra,ra,.1 + .8*rand(1001)*.001);
wave_2_per_point2=rb = if(rb,rb,.1 + .8*rand(1001)*.001);
wave_2_per_point3=rc = if(rc,rc,.1 + .8*rand(1001)*.001);
wave_2_per_point4=rd = if(rd,rd,.1 + .8*rand(1001)*.001);
wave_2_per_point5=
wave_2_per_point6=vol = (value1+value2)*.5;
wave_2_per_point7=vol = 0;
wave_2_per_point8=it = it*above(sample,0);
wave_2_per_point9=it = it + 1;
wave_2_per_point10=
wave_2_per_point11=sp = sample*10;
wave_2_per_point12=ti = q1;
wave_2_per_point13=
wave_2_per_point14=ox = .5*sin(ti*t7 + sp*t1) + .5*sin(ti*rb + sp*t4);
wave_2_per_point15=oy = .5*sin(ti*t8 + sp*t2) + .5*sin(ti*rc + sp*t5);
wave_2_per_point16=oz = .5*sin(ti*ra + sp*t3) + .5*sin(ti*rd + sp*t6);
wave_2_per_point17=
wave_2_per_point18=ox = ox*q5;
wave_2_per_point19=oy = oy*q5;
wave_2_per_point20=oz = oz*q5;
wave_2_per_point21=
wave_2_per_point22=
wave_2_per_point23=xang = q2;
wave_2_per_point24=yang = q3;
wave_2_per_point25=zang = q4;
wave_2_per_point26=
wave_2_per_point27=fov = .5;
wave_2_per_point28=
wave_2_per_point29=mx = ox*cos(yang) + oz*sin(yang);
wave_2_per_point30=mz = - ox*sin(yang) + oz*cos(yang);
wave_2_per_point31=ox = mx;
wave_2_per_point32=oz = mz;
wave_2_per_point33=mx = ox*cos(zang) - oy*sin(zang);
wave_2_per_point34=my = ox*sin(zang) + oy*cos(zang);
wave_2_per_point35=ox = mx;
wave_2_per_point36=oy = my;
wave_2_per_point37=my = oy*cos(xang) - oz*sin(xang);
wave_2_per_point38=mz = oy*sin(xang) + oz*cos(xang);
wave_2_per_point39=oy = my;
wave_2_per_point40=oz = mz;
wave_2_per_point41=
wave_2_per_point42=oz = (oz - int(oz*.2)*5 - 5)*2;
wave_2_per_point43=x = ox*fov/oz + 0.5;
wave_2_per_point44=x = (x-.5)*0.75 + 0.5;
wave_2_per_point45=y = oy*fov/oz + 0.5;
wave_2_per_point46=
wavecode_3_enabled=1
wavecode_3_samples=512
wavecode_3_sep=0
wavecode_3_bSpectrum=1
wavecode_3_bUseDots=0
wavecode_3_bDrawThick=0
wavecode_3_bAdditive=0
wavecode_3_scaling=1.000000
wavecode_3_smoothing=0.000000
wavecode_3_r=1.000000
wavecode_3_g=1.000000
wavecode_3_b=1.000000
wavecode_3_a=1.000000
wave_3_per_frame1=ra = if(ra,ra,2 + 8*rand(1001)*.001);
wave_3_per_frame2=rb = if(rb,rb,2 + 8*rand(1001)*.001);
wave_3_per_frame3=rc = if(rc,rc,2 + 8*rand(1001)*.001);
wave_3_per_frame4=rd = if(rd,rd,2 + 8*rand(1001)*.001);
wave_3_per_frame5=re = if(re,re,2 + 8*rand(1001)*.001);
wave_3_per_frame6=rf = if(rf,rf,2 + 8*rand(1001)*.001);
wave_3_per_frame7=
wave_3_per_frame8=t1 = ra*6.2832;
wave_3_per_frame9=t2 = rb*6.2832;
wave_3_per_frame10=t3 = rc*6.2832;
wave_3_per_frame11=t4 = rd*6.2832;
wave_3_per_frame12=t5 = re*6.2832;
wave_3_per_frame13=t6 = rf*6.2832;
wave_3_per_frame14=
wave_3_per_frame15=rg = if(rg,rg,.1 + .8*rand(1001)*.001);
wave_3_per_frame16=rh = if(rh,rh,.1 + .8*rand(1001)*.001);
wave_3_per_frame17=
wave_3_per_frame18=t7 = rg;
wave_3_per_frame19=t8 = rh;
wave_3_per_frame20=
wave_3_per_frame21=
wave_3_per_frame22=tic = min(time-tir,.1);
wave_3_per_frame23=tir = time;
wave_3_per_frame24=ti = ti + tic*.5 + below(vr+vg+vb,.4)*tic*8;
wave_3_per_frame25=
wave_3_per_point1=ra = if(ra,ra,.1 + .8*rand(1001)*.001);
wave_3_per_point2=rb = if(rb,rb,.1 + .8*rand(1001)*.001);
wave_3_per_point3=rc = if(rc,rc,.1 + .8*rand(1001)*.001);
wave_3_per_point4=rd = if(rd,rd,.1 + .8*rand(1001)*.001);
wave_3_per_point5=
wave_3_per_point6=vol = (value1+value2)*.5;
wave_3_per_point7=vol = 0;
wave_3_per_point8=it = it*above(sample,0);
wave_3_per_point9=it = it + 1;
wave_3_per_point10=
wave_3_per_point11=sp = sample*10;
wave_3_per_point12=ti = q1;
wave_3_per_point13=
wave_3_per_point14=ox = .5*sin(ti*t7 + sp*t1+q2) + .5*sin(ti*rb + sp*t4);
wave_3_per_point15=oy = .5*sin(ti*t8 + sp*t2+q3) + .5*sin(ti*rc + sp*t5);
wave_3_per_point16=oz = .5*sin(ti*ra + sp*t3+q4) + .5*sin(ti*rd + sp*t6);
wave_3_per_point17=
wave_3_per_point18=ox = ox*q5;
wave_3_per_point19=oy = oy*q5;
wave_3_per_point20=oz = oz*q5;
wave_3_per_point21=
wave_3_per_point22=
wave_3_per_point23=xang = q2;
wave_3_per_point24=yang = q3;
wave_3_per_point25=zang = q4;
wave_3_per_point26=
wave_3_per_point27=fov = .5;
wave_3_per_point28=
wave_3_per_point29=mx = ox*cos(yang) + oz*sin(yang);
wave_3_per_point30=mz = - ox*sin(yang) + oz*cos(yang);
wave_3_per_point31=ox = mx;
wave_3_per_point32=oz = mz;
wave_3_per_point33=mx = ox*cos(zang) - oy*sin(zang);
wave_3_per_point34=my = ox*sin(zang) + oy*cos(zang);
wave_3_per_point35=ox = mx;
wave_3_per_point36=oy = my;
wave_3_per_point37=my = oy*cos(xang) - oz*sin(xang);
wave_3_per_point38=mz = oy*sin(xang) + oz*cos(xang);
wave_3_per_point39=oy = my;
wave_3_per_point40=oz = mz;
wave_3_per_point41=
wave_3_per_point42=oz = (oz - int(oz*.2)*5 - 5)*2;
wave_3_per_point43=x = ox*fov/oz + 0.5;
wave_3_per_point44=x = (x-.5)*0.75 + 0.5;
wave_3_per_point45=y = oy*fov/oz + 0.5;
wave_3_per_point46=
wave_3_per_point47=
wave_3_per_point48=r=tan(x*6.28+q2);
wave_3_per_point49=r=min ( max(r*treb,0),1);
wave_3_per_point50=g=tan(y*6.28+2.1+q3);
wave_3_per_point51=g=min ( max(g*mid,0),1);
wave_3_per_point52=b=tan((x+y)*3.14+4.2+q4);
wave_3_per_point53=b=min ( max(b*bass,0),1);
shapecode_0_enabled=0
shapecode_0_sides=4
shapecode_0_additive=0
shapecode_0_thickOutline=1
shapecode_0_textured=1
shapecode_0_x=0.500000
shapecode_0_y=0.500000
shapecode_0_rad=2.008520
shapecode_0_ang=0.000000
shapecode_0_tex_ang=0.000000
shapecode_0_tex_zoom=0.508316
shapecode_0_r=0.900000
shapecode_0_g=0.940000
shapecode_0_b=0.890000
shapecode_0_a=1.000000
shapecode_0_r2=0.840000
shapecode_0_g2=0.930000
shapecode_0_b2=1.000000
shapecode_0_a2=1.000000
shapecode_0_border_r=1.000000
shapecode_0_border_g=1.000000
shapecode_0_border_b=0.000000
shapecode_0_border_a=0.100000
shape_0_init1=t1 = rand(100)*0.01;
shape_0_init2=t2 = rand(100)*0.01;
shape_0_init3=te = 1;
shape_0_init4=poly = 5;
shape_0_per_frame1=ti = time*.1;
shape_0_per_frame2=r = .95 + .05*sin(ti*1.821);
shape_0_per_frame3=g = .95 + .05*sin(ti*1.838);
shape_0_per_frame4=b = .95 + .05*sin(ti*1.868);
shape_0_per_frame5=
shape_0_per_frame6=r2=r;
shape_0_per_frame7=g2=g;
shape_0_per_frame8=b2=b;
shapecode_1_enabled=1
shapecode_1_sides=34
shapecode_1_additive=0
shapecode_1_thickOutline=0
shapecode_1_textured=1
shapecode_1_x=0.500000
shapecode_1_y=0.500000
shapecode_1_rad=0.662308
shapecode_1_ang=0.000000
shapecode_1_tex_ang=0.000000
shapecode_1_tex_zoom=1.503750
shapecode_1_r=1.000000
shapecode_1_g=1.000000
shapecode_1_b=0.000000
shapecode_1_a=1.000000
shapecode_1_r2=1.000000
shapecode_1_g2=0.000000
shapecode_1_b2=1.000000
shapecode_1_a2=0.800000
shapecode_1_border_r=1.000000
shapecode_1_border_g=1.000000
shapecode_1_border_b=1.000000
shapecode_1_border_a=0.100000
shape_1_per_frame1=tex_ang=0.01;
shape_1_per_frame2=a=bass_att;
shapecode_2_enabled=1
shapecode_2_sides=4
shapecode_2_additive=0
shapecode_2_thickOutline=1
shapecode_2_textured=1
shapecode_2_x=0.500000
shapecode_2_y=0.500000
shapecode_2_rad=2.008520
shapecode_2_ang=0.000000
shapecode_2_tex_ang=0.000000
shapecode_2_tex_zoom=0.518531
shapecode_2_r=1.000000
shapecode_2_g=1.000000
shapecode_2_b=1.000000
shapecode_2_a=1.000000
shapecode_2_r2=1.000000
shapecode_2_g2=1.000000
shapecode_2_b2=1.000000
shapecode_2_a2=0.000000
shapecode_2_border_r=1.000000
shapecode_2_border_g=1.000000
shapecode_2_border_b=0.000000
shapecode_2_border_a=0.100000
shape_2_init1=t1 = rand(100)*0.01;
shape_2_init2=t2 = rand(100)*0.01;
shape_2_init3=te = 1;
shape_2_init4=poly = 5;
shape_2_per_frame1=a=treb_att;
shapecode_3_enabled=1
shapecode_3_sides=3
shapecode_3_additive=1
shapecode_3_thickOutline=0
shapecode_3_textured=0
shapecode_3_x=0.500000
shapecode_3_y=0.500000
shapecode_3_rad=1.089253
shapecode_3_ang=0.000000
shapecode_3_tex_ang=0.000000
shapecode_3_tex_zoom=1.000000
shapecode_3_r=1.000000
shapecode_3_g=1.000000
shapecode_3_b=0.000000
shapecode_3_a=0.200000
shapecode_3_r2=0.000000
shapecode_3_g2=0.000000
shapecode_3_b2=0.200000
shapecode_3_a2=0.000000
shapecode_3_border_r=1.000000
shapecode_3_border_g=1.000000
shapecode_3_border_b=1.000000
shapecode_3_border_a=0.200000
shape_3_per_frame1=ang=bass;
per_frame_1=wave_a = 0;
per_frame_2=
per_frame_3=tic = min(time-tin,.1);
per_frame_4=tin = time;
per_frame_5=
per_frame_6=ra = 10;
per_frame_7=treb_avg = tic*(treb_avg*(1/tic - ra) + ra*treb);
per_frame_8=mid_avg = tic*(mid_avg*(1/tic - ra) + ra*mid);
per_frame_9=bass_avg = tic*(bass_avg*(1/tic - ra) + ra*bass);
per_frame_10=vav = tic*(vav*(1/tic - ra) + ra*(bass+treb+mid)*.33333);
per_frame_11=
per_frame_12=tt = tt + tic*treb_avg;
per_frame_13=mt = mt + tic*mid_avg;
per_frame_14=bt = bt + tic*bass_avg;
per_frame_15=vt = vt + tic*vav;
per_frame_16=
per_frame_17=sp = abs(vav - slide)*.1;
per_frame_18=
per_frame_19=slide = if(above(slide,vav),slide-tic*sp,slide+tic*sp);
per_frame_20=
per_frame_21=q1 = vt*.0 + 300;
per_frame_22=q2 = tt*.25;
per_frame_23=q3 = mt*.25;
per_frame_24=q4 = bt*.25;
per_frame_25=q5 = slide*.6*6;
per_frame_26=decay=0.95;
per_frame_27=
per_frame_28=monitor=q3
