Filter buffersink
  Buffer video frames, and make them available to the end of the filter graph.
    Inputs:
       #0: default (video)
    Outputs:
        none (sink filter)
buffersink AVOptions:
  pix_fmts          <binary>     ..FV..... set the supported pixel formats


