Decoder g722 [G.722 ADPCM]:
    General capabilities: dr1 
    Threading capabilities: none
g722 decoder AVOptions:
  -bits_per_codeword <int>        .D..A.... Bits per G722 codeword (from 6 to 8) (default 8)


