Demuxer s16be [PCM signed 16-bit big-endian]:
s16be demuxer AVOptions:
  -sample_rate       <int>        .D.......  (from 0 to INT_MAX) (default 44100)
  -channels          <int>        .D.......  (from 0 to INT_MAX) (default 1)


