Encoder sgi [SGI image]:
    General capabilities: none
    Threading capabilities: none
    Supported pixel formats: rgb24 rgba rgb48le rgb48be rgba64le rgba64be gray16le gray16be gray
sgi AVOptions:
  -rle               <int>        E..V..... Use run-length compression (from 0 to 1) (default 1)


