  To enable the EuSynth Pro/Host  software  go  into  ControlPanel/
System/Device  Manager/Sound,  video and game controllers and select 
the KINGTECH AD1815 Sound  CARD  Controller.     Go to the Properties
/Settings  and  check  the  "Enable  EuSynth  Pro Host box. You must 
restart Windows for the change to take effect.

  For DOS box game support go into ControlPanel/Multimedia/Advanced/
MIDI devices  and  Instruments.  Select  EuSynth/Pro-Host  MIDI/
Properties/Settings... Select The I/O address, IRQ and  DMA channels
as required ( select Help button for additional  information ). 
  We have verified that Descent2 will play using the 
following settings: MPU401 
                 address = 330 
SoundBlaster I/O address = 240 
        SoundBlaster IRQ = 7 
        SoundBlaster DMA = 3
