;	Copyright Trident Microsystems, Inc (c) 1997-1999  All Rights Reserved.
;	Portions Copyright (c) 1993 Microsoft Corporation.  All Rights Reserved.
;
;	Title:    OEMSETUP.INF - Trident PCI Audio Installation File
;       Author:   Tom Warren - Trident Microsystems, Arizona Product Group
;       Updated:  10/29/97 - TRIDWAVE/TRIDWNW name change - TCW APG
;       Updated:  10/30/97 - Fix MIDIMAP wavetable auto-assign - TCW APG
;       Updated:  11/18/97 - Added 4DWave and 9753Wave Rev B
;       Updated:  12/03/97 - Added Autoexec update for WAVEINIT/WAVETSR.
;       Updated:  12/12/97 - Switched midi devices 0 and 1.
;       Updated:  12/19/97 - Fixed Joystick install??, added sample set CD.
;       Updated:  02/12/98 - Removed all LogConfig stuff, not needed.
;       Updated:  02/13/98 - Added QA3D installation code.
;       Updated:  02/20/98 - Added code to install Microsoft Joystick.
;       Updated:  03/18/98 - Added Q3DCTL control program to install & run.
;       Updated:  03/23/98 - Added our own flavor of Joystick.
;       Updated:  03/23/98 - Disabled A3D installation for this release.
;       Updated:  04/01/98 - Added handling of Direct Input installation.
;                            This installs tridinpt.inf and standard joystick.
;       Updated:  04/29/98 - Reenable A3D installation for this release.
;       Updated:  04/29/98 - Remove Q3DCTL, no internationalization support.
;       Updated:  05/12/98 - Added NX support, removed 9753 support.
;       Updated:  06/30/98 - Added TridTray.exe and TridCpl.cpl.
;       Updated:  08/14/98 - Added some PCI strings for NX to ease 98 installs.
;       Updated:  08/31/98 - Modified Legacy device to use mmdevldr,
;                            plus assigned VxD to Legacy as its driver.
;       Updated:  11/18/98 - Added triq3d.exe to the install.
;       Updated:  12/07/98 - Support for NX rev C.
;       Updated:  12/30/98 - Added Support for most common NX EPROM Values.
;       Updated:  01/21/99 - Added lines suport OEM EEPROM SUBSYS_1400122D.
;       Updated:  01/27/99 - Added strings from Mixer, for OEM Customization.
;       Updated:  01/28/99 - Change NX to 2/4 MB Sample Sets only.
;       Updated:  01/29/99 - Proliferated 11 languages
;       Updated:  02/03/99 - Now supports OEM flag field

; Simplified Chinese Version


[Version]
Signature="$CHICAGO$"
Class=MEDIA
Provider=%TMS%
LayoutFile=LAYOUT.INF

[ClassInstall]
AddReg=Class.AddReg

[Class.AddReg]
HKR,,,,%MediaClassName%
HKR,,Icon,,"-1"
HKR,,Installer,,mmci.dll

[Manufacturer]
%TRIDMfgName%=TRID

[TRID]
%PCI\VEN_1023&DEV_2000.DeviceDesc% = TRID4DDX, PCI\VEN_1023&DEV_2000
%PCI\VEN_1023&DEV_2000.DeviceDesc% = TRID4DDX, PCI\VEN_1023&DEV_2000&SUBSYS_20001023&REV_02
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001
; Windows 98.  Add more lines for each OEM's SubSys ID when available.
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_FFFFFFFF&REV_00
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_00000000&REV_01
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_0000FFFF&REV_01
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_FFFF0000&REV_01
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_FFFFFFFF&REV_01
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_20011023&REV_01
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_00000000&REV_02
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_0000FFFF&REV_02
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_FFFF0000&REV_02
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_FFFFFFFF&REV_02
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_20011023&REV_02
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_1400122D&REV_02
%PCI\VEN_1023&DEV_2001.DeviceDesc% = TRID4DNX, PCI\VEN_1023&DEV_2001&SUBSYS_1400122D
%Trident_Legacy_Device.DeviceDesc% = Trid_Legacy.Install,VIRTUAL\Trid_Legacy

[TRID4DDX]
CopyFiles=TRID_SysCopyFiles, TRIDDX_SampleSets
UpdateInis=TRID_UpdateInis
AddReg=WAVE.AddReg, MIXER.AddReg, TRID4DDX.AddReg, TRAY.AddReg, QA3D.AddReg 
UpdateAutoBat=TRID_Update_Autobat

[TRID4DNX]
CopyFiles=TRID_SysCopyFiles, TRIDNX_SampleSets
UpdateInis=TRID_UpdateInis
AddReg=WAVE.AddReg, MIXER.AddReg, TRID4DNX.AddReg, TRAY.AddReg, QA3D.AddReg 
UpdateAutoBat=TRID_Update_Autobat

;---------------------------------------------------------------;
[PreCopySection]
HKR,,NoSetupUI,,1

[Det.DevINFs]
VIRTUAL\Trid_Gameport=tridinpt.inf

;---------------------------------------------------------------;

[TRID_SysCopyFiles]
TRIDWNW.VXD
TRIDWAVE.DRV
TRIDCPL.CPL
TRIDTRAY.EXE
WAVEINIT.EXE
WAVETSR.COM
QHOOK.VXD
QA3D.DLL
A3D.DLL
QA3DLOAD.DLL
TRIQ3D.EXE

[TRIDNX_SampleSets]
GM10MB.SLB
GM15MB.SLB
GM20MB.SLB
GM60MB.SLB
;GMNX20MB.SLB
;GMNX40MB.SLB

[TRIDDX_SampleSets]
GM10MB.SLB
GM15MB.SLB
GM20MB.SLB
GM60MB.SLB

[TRID_UpdateInis]
system.ini,drivers,"midi=TRIDWAVE.DRV",,0
system.ini,drivers,"mixer=TRIDWAVE.DRV",,0
system.ini,drivers,"wave=TRIDWAVE.DRV",,0
system.ini,drivers,"aux=TRIDWAVE.DRV",,0
system.ini,drivers,"joystick="

[TRID_Update_AutoBat]
;CmdAdd=WAVEINIT.EXE,"/v"
;CmdAdd=WAVETSR.COM

[DestinationDirs]
TRID_SysCopyFiles = 11 ; 	System Directory
TRID_WinCopyFiles = 10 ;	Windows Directory
DefaultDestDir=11

[WAVE.AddReg]
HKR,,DevLoader,,mmdevldr.vxd
HKLM,%KEY_IOC%\acm,,,
HKLM,%KEY_IOC%\Rec,,,
HKLM,%KEY_IOC%\MPlay,,,
; OEM Aztech
;HKR,%OEM%,OEMSelect,1,01,00,00,00
; OEM Trident
HKR,%OEM%,OEMSelect,1,00,00,00,00

[MIXER.AddReg]
HKLM,%KEY_RUN%,SystemTray,,"SysTray.Exe"
HKLM,%KEY_IOC%\Vol,,,


;** MIXER_VOLUME Settings.
; Do not change these names, as they are used by the driver
;
HKR,%CONFIG%,LineoutVolMute,1,00,00,00,00
HKR,%CONFIG%,HeadphoneVolMute,1,00,00,00,00
HKR,%CONFIG%,MonooutVolMute,1,00,00,00,00
HKR,%CONFIG%,LineInVolMute,1,00,00,00,00
HKR,%CONFIG%,MidiVolMute,1,00,00,00,00
HKR,%CONFIG%,CDVolMute,1,00,00,00,00
HKR,%CONFIG%,MonoMICVolMute,1,00,00,00,00
HKR,%CONFIG%,WaveVolMute,1,00,00,00,00
HKR,%CONFIG%,PCBeepVolMute,1,00,00,00,00
HKR,%CONFIG%,AUXVolMute,1,00,00,00,00
HKR,%CONFIG%,VideoVolMute,1,00,00,00,00
HKR,%CONFIG%,PhoneVolMute,1,00,00,00,00
HKR,%CONFIG%,PCMVolMute,1,00,00,00,00
HKR,%CONFIG%,LeftLineoutVol,1,ff,df,00,00
HKR,%CONFIG%,RightLineoutVol,1,ff,df,00,00
HKR,%CONFIG%,LeftHeadphoneVol,1,ff,ff,00,00
HKR,%CONFIG%,RightHeadphoneVol,1,ff,ff,00,00
HKR,%CONFIG%,MonooutVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftLineInVol,1,ff,ff,00,00
HKR,%CONFIG%,RightLineInVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftMidiVol,1,ff,ff,00,00
HKR,%CONFIG%,RightMidiVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftCDVol,1,ff,ff,00,00
HKR,%CONFIG%,RightCDVol,1,ff,ff,00,00
HKR,%CONFIG%,MonoMICVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftWaveVol,1,ff,ff,00,00
HKR,%CONFIG%,RightWaveVol,1,ff,ff,00,00
HKR,%CONFIG%,MonoPCBeepVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftAUXVol,1,ff,ff,00,00
HKR,%CONFIG%,RightAUXVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftVideoVol,1,ff,ff,00,00
HKR,%CONFIG%,RightVideoVol,1,ff,ff,00,00
HKR,%CONFIG%,MonoPhoneVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftPCMVol,1,00,c0,00,00
HKR,%CONFIG%,RightPCMVol,1,00,c0,00,00
HKR,%CONFIG%,LeftWaveInLineInVol,1,ff,ff,00,00
HKR,%CONFIG%,RightWaveInLineInVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftWaveInCDVol,1,ff,ff,00,00
HKR,%CONFIG%,RightWaveInCDVol,1,ff,ff,00,00
HKR,%CONFIG%,WaveInMicVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftWaveInAUXVol,1,ff,ff,00,00
HKR,%CONFIG%,RightWaveInAUXVol,1,ff,ff,00,00
HKR,%CONFIG%,LeftWaveInVideoVol,1,ff,ff,00,00
HKR,%CONFIG%,RightWaveInVideoVol,1,ff,ff,00,00
HKR,%CONFIG%,WaveInPhone,1,ff,ff,00,00
HKR,%CONFIG%,LeftWaveInStereoMix,1,ff,ff,00,00
HKR,%CONFIG%,RightWaveInStereoMix,1,ff,ff,00,00
HKR,%CONFIG%,WaveInMonoMix,1,ff,ff,00,00
HKR,%CONFIG%,WaveInSource,="LineIn"
HKR,%CONFIG%,MonoOutSource,="MonoMix"
HKR,%CONFIG%,ToneBass,1,ff,ff,00,00
HKR,%CONFIG%,ToneTreble,1,ff,ff,00,00
HKR,%CONFIG%,MonoMix,1,ff,ff,00,00
HKR,%CONFIG%,Microphone,1,ff,ff,00,00


;** MIXER_LABEL_SETINGS
; Constraints on labels:
; LONG labels can be up to 64 characters long, including the null terminator
; SHORT labels can be up to 16 characters long, including the null terminator
;
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE0_LONG,, "输入"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE1_LONG,, "MIDI"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE2_LONG,, "CD音响"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE3_LONG,, "麦克风"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE4_LONG,, "音波"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE5_LONG,, "PC喇叭"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE6_LONG,, "辅助输入"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE7_LONG,, "图像 "
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE8_LONG,, "耳机"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE9_LONG,, "StereoMix"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE10_LONG,, "MonoMix"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE11_LONG,, "PCMOut"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE0_SHORT,, "LineIn"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE1_SHORT,, "MIDI"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE2_SHORT,, "CD"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE3_SHORT,, "麦克风"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE4_SHORT,, "音波"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE5_SHORT,, "喇叭"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE6_SHORT,, "辅助输入"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE7_SHORT,, "图像"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE8_SHORT,, "耳机"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE9_SHORT,, "StereoMix"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE10_SHORT,, "MonoMix"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_SOURCE11_SHORT,, "PCM"

HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_DEST0_LONG,, "主音量控制"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_DEST1_LONG,, "主音量控制"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_DEST2_LONG,, "MonoOut Control"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_DEST0_SHORT,, "播放"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_DEST1_SHORT,, "录音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_DEST2_SHORT,, "MonoOut"

HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL0_LONG,, "Trident PCI 输出的输入音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL1_LONG,, "Trident PCI 输出的音乐输出音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL2_LONG,, "Trident PCI 输出的CD输出音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL3_LONG,, "Trident PCI 输出的麦克风音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL4_LONG,, "Trident PCI 输出的音波输出音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL5_LONG,, "Trident PCI 输出的PC喇叭音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL6_LONG,, "Trident PCI 输出的辅助输入音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL7_LONG,, "Trident PCI 输出的图像音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL8_LONG,, "Trident PCI 输出的耳机音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL9_LONG,, "Trident PCI 输出的输入静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL10_LONG,, "Trident PCI 输出的音乐输出静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL11_LONG,, "Trident PCI 输出的CD输出静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL12_LONG,, "Trident PCI 输出的麦克风静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL13_LONG,, "Trident PCI 输出的音波输出静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL14_LONG,, "Trident PCI 输出的PC喇叭信号静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL15_LONG,, "Trident PCI 输出的辅助输入静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL16_LONG,, "Trident PCI 输出的影像静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL17_LONG,, "Trident PCI 输出的耳机静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL18_LONG,, "Trident PCI 录音的输入音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL19_LONG,, "Trident PCI 录音的CD输出音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL20_LONG,, "Trident PCI 录音的麦克风音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL21_LONG,, "Trident PCI 录音的辅助输入音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL22_LONG,, "Trident PCI 录音的音像音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL23_LONG,, "Trident PCI 录音的耳机音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL24_LONG,, "Trident PCI 录音的立体混音音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL25_LONG,, "Trident PCI 录音的单体混音音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL26_LONG,, "Trident PCI 录音MUX形音源输入选择器"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL27_LONG,, "Trident PCI 输出的主音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL28_LONG,, "Trident PCI 耳机输出的主音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL29_LONG,, "Trident PCI 单音输出的主音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL30_LONG,, "Trident PCI 输出的静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL31_LONG,, "Trident PCI 耳机输出的静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL32_LONG,, "Trident PCI 单音输出的静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL33_LONG,, "Trident PCI 输出的低音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL34_LONG,, "Trident PCI 输出的高音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL35_LONG,, "Trident PCI MonoOut MonoMix"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL36_LONG,, "Trident PCI MonoOut Microphone"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL37_LONG,, "Trident PCI 音波输出的强度表"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL38_LONG,, "Trident PCI 输出入的一般控制"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL39_LONG,, "Trident PCI 输出的音量"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL40_LONG,, "Trident PCI 输出的静音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL41_LONG,, "Trident PCI MonoOut Input MUX Type Source Selector"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL42_LONG,, "付捞农 20dB 何胶飘"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL43_LONG,, "付捞农 20dB 何胶飘"

HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL0_SHORT,, "LineInVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL1_SHORT,, "MidiVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL2_SHORT,, "CDVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL3_SHORT,, "MicVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL4_SHORT,, "WaveVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL5_SHORT,, "PcBpVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL6_SHORT,, "AUXVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL7_SHORT,, "VideoVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL8_SHORT,, "PhoneVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL9_SHORT,, "LineInMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL10_SHORT,, "MidiMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL11_SHORT,, "CDMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL12_SHORT,, "MicMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL13_SHORT,, "WaveMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL14_SHORT,, "PcBpMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL15_SHORT,, "AUXMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL16_SHORT,, "VideoMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL17_SHORT,, "PhoneMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL18_SHORT,, "LineInVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL19_SHORT,, "CDVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL20_SHORT,, "MicVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL21_SHORT,, "AUXVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL22_SHORT,, "VideoVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL23_SHORT,, "PhoneVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL24_SHORT,, "StereoVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL25_SHORT,, "MonoVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL26_SHORT,, "WaveInMux"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL27_SHORT,, "LineOutVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL28_SHORT,, "HdphOutVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL29_SHORT,, "MonoOutVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL30_SHORT,, "LineOutVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL31_SHORT,, "HdphOutVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL32_SHORT,, "MonoOutVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL33_SHORT,, "低音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL34_SHORT,, "高音"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL35_SHORT,, "MonoMix"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL36_SHORT,, "Microphone"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL37_SHORT,, "WaveOutPM"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL38_SHORT,, "GeneralPP"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL39_SHORT,, "PCMOutVol"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL40_SHORT,, "PCMOutMute"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL41_SHORT,, "MonoOutMux"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL42_SHORT,, "付捞农 20dB 何胶飘"
HKR,%MIXER_LABEL_SETTINGS%,SR_STR_MIXER_CONTROL43_SHORT,, "付捞农 20dB 何胶飘"


[TRID4DDX.AddReg]
HKR,,Driver,,TRIDWNW.VXD
HKR,Drivers,MIGRATED,,1
HKR,Drivers\midi,,,
HKR,Drivers\wave,,,
HKR,Drivers\mixer,,,
HKR,Drivers\aux,,,
HKR,Drivers\wave\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\mixer\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\aux\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\wave\TRIDWAVE.DRV,Description,,%PCI\VEN_1023&DEV_2000.DeviceDesc%
HKR,Drivers\mixer\TRIDWAVE.DRV,Description,,%PCI\VEN_1023&DEV_2000.DeviceDesc%
HKR,Drivers\aux\TRIDWAVE.DRV,Description,,%PCI\VEN_1023&DEV_2000.DeviceDesc%
;***
HKR,Drivers\wave\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\mixer\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\aux\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
;***
HKR,Drivers\midi\%V_WAVETABLE%,Driver,,TRIDWAVE.DRV
HKR,Drivers\midi\%V_WAVETABLE%,Description,,%V_WAVETABLE%
HKR,Drivers\midi\%V_WAVETABLE%,NumPorts,1,02,00,00,00
HKR,Drivers\midi\%V_WAVETABLE%,Port,1,00,00,00,00
;***
HKR,Drivers\midi\%V_EXTERNAL%,Driver,,TRIDWAVE.DRV
HKR,Drivers\midi\%V_EXTERNAL%,Description,,%V_EXTERNAL%
HKR,Drivers\midi\%V_EXTERNAL%,NumPorts,1,02,00,00,00
HKR,Drivers\midi\%V_EXTERNAL%,Port,1,01,00,00,00
;***
HKR,Drivers,SubClasses,,"wave,midi,aux,mixer"
HKR,%SETTINGS%,,,
HKR,,EnumPropPages,,"TRIDWAVE.DRV,DrvEnumPropPages"

[TRID4DNX.AddReg]
HKR,,Driver,,TRIDWNW.VXD
HKR,Drivers,MIGRATED,,1
HKR,Drivers\midi,,,
HKR,Drivers\wave,,,
HKR,Drivers\mixer,,,
HKR,Drivers\aux,,,
HKR,Drivers\wave\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\mixer\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\aux\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\wave\TRIDWAVE.DRV,Description,,%PCI\VEN_1023&DEV_2001.DeviceDesc%
HKR,Drivers\mixer\TRIDWAVE.DRV,Description,,%PCI\VEN_1023&DEV_2001.DeviceDesc%
HKR,Drivers\aux\TRIDWAVE.DRV,Description,,%PCI\VEN_1023&DEV_2001.DeviceDesc%
;***
HKR,Drivers\wave\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\mixer\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
HKR,Drivers\aux\TRIDWAVE.DRV,Driver,,TRIDWAVE.DRV
;***
HKR,Drivers\midi\%V_WAVETABLE%,Driver,,TRIDWAVE.DRV
HKR,Drivers\midi\%V_WAVETABLE%,Description,,%V_WAVETABLE%
HKR,Drivers\midi\%V_WAVETABLE%,NumPorts,1,02,00,00,00
HKR,Drivers\midi\%V_WAVETABLE%,Port,1,00,00,00,00
;***
HKR,Drivers\midi\%V_EXTERNAL%,Driver,,TRIDWAVE.DRV
HKR,Drivers\midi\%V_EXTERNAL%,Description,,%V_EXTERNAL%
HKR,Drivers\midi\%V_EXTERNAL%,NumPorts,1,02,00,00,00
HKR,Drivers\midi\%V_EXTERNAL%,Port,1,01,00,00,00
;***
HKR,Drivers,SubClasses,,"wave,midi,aux,mixer"
HKR,%SETTINGS%,,,
HKR,,EnumPropPages,,"TRIDWAVE.DRV,DrvEnumPropPages"

[TRAY.AddReg]
HKLM,%KEY_RUN%,TridTray,,%11%\tridtray.exe" 

[QA3D.AddReg]
HKCR,A3D,,0,A3d Object
HKCR,A3D\CLSID,,0,{d8f1eee0-f634-11cf-8700-00a0245d918b}
HKCR,CLSID\{d8f1eee0-f634-11cf-8700-00a0245d918b},,0,A3d Object
HKCR,CLSID\{d8f1eee0-f634-11cf-8700-00a0245d918b}\InprocServer32,,0,a3d.dll
HKCR,CLSID\{d8f1eee0-f634-11cf-8700-00a0245d918b}\InprocServer32,ThreadingModel,0,Apartment
;HKLM,%KEY_RUN%,Q3DControlPanel,,%11%\q3dctl.exe" 


;---------------------------------------------------------------;

[Trid_Legacy.Install]
AddReg=Trid_Legacy.AddReg

[Trid_Legacy.AddReg]
HKR,,DevLoader,,mmdevldr.vxd
HKR,,Driver,,tridwnw.vxd
HKR,Drivers,MIGRATED,,0
HKR,,EnumPropPages,,"EnumPropPages"

[SourceDisksFiles]
TRIDWNW.VXD=2
TRIDWAVE.DRV=2
TRIDCPL.CPL=2
TRIDTRAY.EXE=2
WAVEINIT.EXE=2
WAVETSR.COM=2
QHOOK.VXD=2
QA3D.DLL=2
A3D.DLL=2
QA3DLOAD.DLL=2
TRIQ3D.EXE=2
GMNX20MB.SLB=2
GMNX40MB.SLB=2
GM10MB.SLB=2
GM15MB.SLB=2
GM20MB.SLB=2
GM60MB.SLB=2

[SourceDisksNames]
1=%DirectX5CD%,%DirectX5%,0
2=%AudioInstallCD%,,

[Strings]
;Non-localized strings
KEY_WARNVER="SYSTEM\CurrentControlSet\Control\SessionManager\WarnVerDLLs"
KEY_CHKVER="SYSTEM\CurrentControlSet\Control\SessionManager\CheckVerDLLs"
KEY_FIL="SYSTEM\CurrentControlSet\Control\MediaResources\FilterList"
KEY_IOC="SYSTEM\CurrentControlSet\Control\MediaResources\InstallOptionalComponents"
KEY_RUN="Software\Microsoft\Windows\CurrentVersion\Run"
KEY_OEM="System\CurrentControlSet\Control\MediaProperties\PrivateProperties\Joystick\OEM\Trident GameCard"
CONFIG="Config"
SETTINGS="Settings"
OEM="OEM"

;Localized strings
TMS="Trident Microsystems, Inc. APG"
TRIDMfgName="TRID"
DirectX5CD="DirectX 5.0 Drivers Redist"
DirectX5="DirectX5.0"
AudioInstallCD="Trident PCI Audio Driver Install CD"
MediaClassName="Sound, video and game controllers"
PCI\VEN_1023&DEV_2000.DeviceDesc="Trident 4DWave(DX) PCI Audio"
PCI\VEN_1023&DEV_2001.DeviceDesc="Trident 4DWave(NX) PCI Audio"
Trident_Legacy_Device.DeviceDesc="Trident Legacy Audio"
V_WAVETABLE="Trident PCI WaveTable MIDI"
V_EXTERNAL="Trident PCI External MIDI"
Trident_Joystick.DeviceDesc="Trident Gameport"
GameCard.DeviceDesc="Trident Direct Input Driver"
MIXER_LABEL_SETTINGS="Settings\MixerLabels"

; **** End of OEMSETUP.INF ****
