The OS/2 Service Pak CDROM
--------------------------

This CDROM contains both the OS/2 2.0 Service Pak (XR06055) and the
OS/2 1.3x Extended Edition Service Pak (XR05100), as well as a series of
fixes to allow OS/2 1.3x Extended Edition to be installed on the
IBM PS/2 95xx and IBM PS/VP series of machines. Also included is the IBM C
Set/2 compiler CSD 28.

Full details of the Service Paks and fixes are given in the subsequent
sections of this document. Additional, and important, information is
provided in documentation files that accompany each series of fixes or
Service Pak. YOU MUST READ OR PRINT THESE DOCUMENTATION FILES BEFORE YOU
ATTEMPT TO INSTALL ANY SERVICE PAK OR FIX.

NOTE: * References in any documentation files on this CDROM to EMTCOPY
        should be ignored. The DSK4PM.EXE utility supplied on this CDROM
        (see the section 'Creating Diskettes from Image Files') is
        functionally equivalent to EMTCOPY for the creation of diskettes
        from the supplied image files. This program requires OS/2 1.2 or
        greater to operate.




The OS/2 1.3x Fix Files for PS/2 95xx and PS/VP
-----------------------------------------------

The diskettes and fix files for the following language versions of
OS/2 1.3x are contained in the following directories on this CDROM:

        DANISH          - \13FIXES\DENMARK      (2 diskette images)
        FRENCH          - \13FIXES\FRANCE       (2 diskette images)
        GERMAN          - \13FIXES\GERMANY      (2 diskette images)
        ITALIAN         - \13FIXES\ITALY        (2 diskette images)
        DUTCH           - \13FIXES\DUTCH        (2 diskette images)
        NORWEGIAN       - \13FIXES\NORWAY       (2 diskette images)
        PORTUGESE       - \13FIXES\PORTUGAL     (2 diskette images)
        SPANISH         - \13FIXES\SPAIN        (2 diskette images)
        FINNISH         - \13FIXES\FINLAND      (2 diskette images)
        SWEDISH         - \13FIXES\SWEDEN       (2 diskette images)
        UNITED KINGDOM  - \13FIXES\UK           (2 diskette images)

Each of the language directories contains 2 diskette images (replacement
installation diskettes for both OS/2 1.31 and OS/2 1.32), replacement
BASEDD02.SYS file for OS/2 1.31 and a replacement BASEDD01.SYS file for
OS/2 1.31 and OS/2 1.32. Full instructions on these fixes are contained
in a documentation file (with an extension of .DOC) WHICH MUST BE READ
PRIOR TO APPLYING THESE FIXES.

All diskettes images provided are for 3.5" diskette drives only. DO NOT
ATTEMPT TO CREATE THE DISKETTES AS 5.25", AS THIS WILL NOT WORK.

See the section of this document called 'Creating Diskettes from
Image Files' for instructions on creating the diskettes from the image
files supplied. The BASEDD0x files can be copied directly from the CDROM.

NOTES: * If you wish to install OS/2 1.3x Extended Editon on either an IBM
         PS/2 95xx machine, or an IBM PS/VP machine, then you will need to
         apply these fixes BEFORE you begin you installation. Choose the
         language version that corresponds with the language version of
         OS/2 1.3x Extended Edition you have, and then read the
         documentation file carefully before proceeding with the
         installation.

       * DO NOT mix different language versions of the fixes with the
         language version of OS/2 1.3x Extended Edition that you have. This
         may cause unpredictable or damaging results.

       * Where you are told to replace files on the OS/2 1.3x Extended
         Edition diskettes, DO MAKE BACKUPS of the files you replace
         BEFORE you replace them.

       * THESE FIXES ARE DESIGNED FOR OS/2 1.3X EXTENDED EDITION ONLY.
         Attempts to apply them to OS/2 1.3x Standard Editon may cause
         unpredictable or damaging results.




The OS/2 1.3 Extended Edition Service Pak XR05100
-------------------------------------------------

The diskettes for the following language versions of the OS/2 1.3 Extended
Edition Service Pak (XR5100) are contained in the following directories on
this CDROM:

        DANISH          - \SP5100\DENMARK      (8 diskette images)
        GERMAN          - \SP5100\GERMANY      (8 diskette images)
        UNITED KINGDOM  - \SP5100\UK           (8 diskette images)

Each of these language directories contains diskette images files (denoted
by the extension .3Hx where x is the diskette number in hexidecimal) and a
documentation file (with the extension .DOC). YOU MUST READ THIS
DOCUMENTATION FILE BEFORE YOU ATTEMPT TO CREATE THE SERVICE PAK DISKETTES
AND INSTALL IT ON YOUR MACHINE.

All diskettes images provided are for 3.5" diskette drives only. DO NOT
ATTEMPT TO CREATE THE DISKETTES AS 5.25", AS THIS WILL NOT WORK.

See the section of this document called 'Creating Diskettes from
Image Files' for instructions on creating the diskettes from the image
files supplied.

NOTES: * DO NOT attempt to install this Service Pak on a machine that does
         not already have OS/2 1.3 Extended Edition installed at level
         5050. This can be checked by typing SYSLEVEL at an OS/2 command
         prompt.

       * DO NOT attempt to install this Service Pak on a machine that has
         only OS/2 1.3 Standard Edition installed on it.

       * DO NOT attempt to install this Service Pak on a machine that has a
         different language version of OS/2 1.3 Extended Edition already
         installed on it. This may cause unpredictable or damaging results.




The OS/2 2.0 Service Pak XR06055
--------------------------------

The diskettes for the following language versions of the Service Pak
(XR6055) are contained in the following directories on this CDROM:

        DANISH          - \SP6055\DENMARK      (15 diskette images)
        DUTCH           - \SP6055\DUTCH        (15 diskette images)
        FINLAND         - \SP6055\FINLAND      (16 diskette images)
        FRENCH          - \SP6055\FRANCE       (15 diskette images)
        GERMAN          - \SP6055\GERMANY      (15 diskette images)
        ITALIAN         - \SP6055\ITALY        (15 diskette images)
        NORWEGIAN       - \SP6055\NORWAY       (15 diskette images)
        PORTUGESE       - \SP6055\PORTUGAL     (15 diskette images)
        SPANISH         - \SP6055\SPAIN        (15 diskette images)
        SWEDISH         - \SP6055\SWEDEN       (15 diskette images)
        UNITED KINGDOM  - \SP6055\UK           (15 diskette images)

Each of these language directories contains diskette images files (denoted
by the extension .3Hx where x is the diskette number in hexidecimal) and a
documentation file (with the extension .DOC). YOU MUST READ THIS
DOCUMENTATION FILE BEFORE YOU ATTEMPT TO CREATE THE SERVICE PAK DISKETTES
AND INSTALL IT ON YOUR MACHINE.

All diskettes images provided are for 3.5" diskette drives only. DO NOT
ATTEMPT TO CREATE THE DISKETTES AS 5.25", AS THIS WILL NOT WORK.

See the section of this document called 'Creating Diskettes from Image
Files' for instructions on creating the diskettes from the image files
supplied.

NOTES: * DO NOT attempt to install this Service Pak on a machine that does
         not already have OS/2 2.0 installed.

       * DO NOT attempt to install this Service Pak on a machine that has
         OS/2 2.00.1 pre-installed on it. This Service Pak is not designed
         to be applied to pre-installed system units, and should refuse to
         work with such systems.

       * DO NOT attempt to install this Service Pak on a machine that has a
         different language version of OS/2 2.0 already installed on it.
         This may cause unpredictable or damaging results.

In addition to these Service Paks on this CDROM, there is also a directory
containing minor updates to the Service Pak XR06055. These fixes reside in
the \SP6055\FIXES directory. They should be unpacked using the PKZIP series
of utilities (not supplied on this CDROM) and any instructions for
installation followed carefully. These fixes are independant of the
language version of the Service Pak you have installed. YOU MUST INSTALL
THE SERVICE PAK BEFORE YOU APPLY ANY OF THESE FIXES.



Creating the C Set/2 CSD Diskettes
----------------------------------

The diskette images for the C Set/2 CSD level 28 are in the \CSET directory
on this CDROM. It consists of the following two image files:

        CSET2V28.3H1 - C Set/2 CSD level 28 diskette 1
        CSET2V28.3H2 - C Set/2 CSD level 28 diskette 2

All diskettes images provided are for 3.5" diskette drives only. DO NOT
ATTEMPT TO CREATE THE DISKETTES AS 5.25", AS THIS WILL NOT WORK.

See the section of this document called 'Creating Diskettes from Image
Files' for instructions on creating the diskettes from the image files
supplied.




Creating the Service Pak
------------------------

CDROM Access
------------

A diskette builder application is supplied on this CDROM to enable you to
turn the diskette images supplied into diskettes. This application will
only run under OS/2 Presentation Manager. If you do not yet have a device
driver that can access your CDROM from OS/2 2.0, then it is suggested that
you copy the appropriate directories from the CDROM onto a hard drive
(accessable from OS/2) using DOS and a suitable CDROM driver. You can then
create the diskettes directly from the hard drive instead of from the CDROM
(the following diskette creation instructions should be followed,
substituting the hard drive for the CDROM drive).


Creating Diskettes from Image Files
-----------------------------------

In the BUILD\ directory on the CDROM, there are the following files :

        DSK4PM.EXE      - Presentation Manager diskette builder
        DSK4PM.HLP      - Help for the DSK4PM program

The DSK4PM.EXE file should be copied from this directory into a directory
that is on your PATH. The DSK4PM.HLP file should be copied into a directory
that is on your HELP path.

This program can be invoked from either the command line (type: DSK4PM
<enter>) or can be placed on your PM desktop and run by double-clicking on
it.

Before you create the diskettes for any one language version of the Service
Pak, you must read the .DOC file in the language directory. This file is a
plain ASCII file containing information about the Service Pak, and the
diskettes that make up the Service Pak.

Once you have read the .DOC file in the language directory, you are ready
to start to create the diskettes for that Service Pak:

 a) Invoke the DSK4PM application. When it has been started, select the
    'Build' option from the menu bar. From the pulldown menu, select the
    diskette drive on which you wish to create the diskettes.

 b) Select the appropriate diskette drive, and you will be presented with a
    dialog box. At this stage, you should ensure that the 'Drive' and
    'Directory' are correct for the CDROM drive and the language directory
    for the Service Pak diskettes that you intend to create.

 c) You can now start creating all the diskettes for the Service Pak. You
    can do this by selecting each diskette image one at a time, or by doing
    a multiple selection on all diskette images at once (be aware that the
    order of the diskette images in the listbox may not match the actual
    order of the diskettes for the Service Pak. Check the .DOC file in the
    directory on the diskette image names to be sure you create them
    correctly).

       * Do NOT try to create a diskette out of the .DOC file. Be sure that
         it is not selected, as the DSK4PM application will reject it.

       * All diskette images have the extension.3Hy (where y is the
         diskette image number of the diskette image file).

Once you have created all the appropriate diskettes from the image files,
you are ready to install the Service Pak on your machine. Before doing
this, you should make suitable backup copies of your CONFIG.SYS file, your
.INI files (in the OS2\ directory on your bootup drive) and you
AUTOEXEC.BAT file.

To start the installation of the Service Pak, simply insert the Service Pak
Installation diskette and reboot your machine. Follow all instructions
carefully.

