;;  MODULE_ID PLPCCW.INM
;;  CalComp AutoCAD 12,13 x86 ADI 4.2 Driver 
;;  Release 6.50  1 Mar 1997 
;;  (C) 1995,1996  CalComp, Inc.
;;  All Rights Reserved.
;; Internationalize these

[DriverMessages]
NumMsgs=14
Msg000=ADI 4.2 driver requires R12 AutoCAD and later.\n
Msg001=ADI 4.2 driver requires R12 AutoCAD and later.\n
Msg002=\nAvailable serial protocols\n
Msg003=0 = ACKNAK\n1 = XON/XOFF\n2 = HARDWARE\n
Msg004=Enter protocol number
Msg005=\nAvailable Baud rates are 9600 or 19200\n
Msg006=Enter the serial baud rate
Msg007=\nAvailable character framing\n
Msg008=0 = 7,E,1\n1 = 8,n,1\n
Msg009=\nEnter character framing number
Msg010=\nFor Detail configurations\n
Msg011=Enter CCONFIG at the AutoCAD 'Command:' prompt\n
Msg012=Select the Model and Configuration to change\n\n
Msg013=\nValid stepsizes are:
Msg014=Enter the number of plotter-steps per inch
Msg015=\nWould you like to change Sync, EOB, and Checksum
Msg016=\nEnter decimal values not hexadecimal values.
Msg017=\nThe current sync code is %d 
Msg018=\nEnter the Sync code
Msg019=\nThe current number of sync codes is %d 
Msg020=\nEnter the number of Sync codes
Msg021=\nThe current EOB is %d 
Msg022=\nEnter the EOB
Msg023=\nDo you want Checksum enabled
Msg024=\nNo response from controller. 
Msg025=To cancel plot, type Control-C : 

[Classes]
NumClasss=5
Class000= CalComp TechJET Ink Jet Plotters     ADI 4.2 V6.50 - by CalComp
Class001= CalComp Pen Plotters                 ADI 4.2 V6.50 - by CalComp
Class002= CalComp Electrostatic Plotters       ADI 4.2 V6.50 - by CalComp
Class003= CalComp DrawingMaster Plotters       ADI 4.2 V6.50 - by CalComp
Class004= CalComp Solus 4 LED Plotters         ADI 4.2 V6.50 - by CalComp
Class005= CalComp TechJET Ink Jet Plotters     ADI 4.2 V6.50 - by CalComp

;; Plotter Parameters
;;  5 Options  - 
;;   0x1001 COMPEN (MULTPEN+MULT2)
;;   0x1801 COMPEN+LONGAXIS 
;;   0x0119 COMMON (MULTPEN+PENWID+VARINC+SFILLS) 
;;   0x0919 COMMON+LONGAXIS
;;  9 Port -
;;   1 SERIAL 2 PARALLEL 3 SERIAL+PARALLEL
;; 15 Features - 
;;   0x0008 HASCDCL 
;;   0x0080 INDEX 
;;   0x0088 HASCDCL+INDEX 
;;   0x0211 PALETTE+MULTICOPY+HASSEQOV
;;   0x0213 PALETTE+HASCOLOR+MULTICOPY+HASSEQOV
;;   0x023D PALETTE+PENMAP+HASCDCL+MULTICOPY+CDCLT+HASSEQOV
;;   0x028D PALETTE+PENMAP+HASCDCL+INDEX+HASSEQOV
;;   0x030F PALETTE+HASCOLOR+PENMAP+HASCDCL+HASCDCLP+HASSEQOV
;;   0x031D PALETTE+PENMAP+HASCDCL+MULTICOPY+HASCDCLP+HASSEQOV
;;   0x031F PALETTE+HASCOLOR+PENMAP+HASCDCL+MULTICOPY+HASCDCLP+HASSEQOV
;;   0x033D PALETTE+PENMAP+HASCDCL+MULTICOPY+CDCLT+HASCDCLP+HASSEQOV
;;   0x035D PALETTE+PENMAP+HASCDCL+MULTICOPY+SROLL+HASCDCLP+HASSEQOV
;; plotter=mname |tag pl_xmax pl_ymax pl_xinc pl_yinc options npens maxspd lines type baud parity data stop handshake features 

[ CalComp TechJET Ink Jet Plotters     ADI 4.2 V6.50 - by CalComp]
NumPlotters=9
Plotter000=*TechJET 175i 5336i, E/A0              |CCP000 182.0 35.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x030F
Plotter001=*TechJET 5524, D/A1                    |CCP000 182.0 24.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x030F
Plotter002=*TechJET 5536, E/A0                    |CCP000 182.0 35.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x030F
Plotter003=*TechJET 175i 5336i, E/A0              |CCP000 182.0 35.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x030F
Plotter004=*TechJET Color 5324, D/A1              |CCP000 182.0 23.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x030F
Plotter005=*TechJET Color 5336, E/A0              |CCP000 182.0 35.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x030F
Plotter006=*TechJET 720c 5624, D/A1               |CCP000 182.0 24.725 360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x028D
Plotter007=*TechJET 720c 5636, E/A0               |CCP000 182.0 35.85  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x028D
Plotter008=*TechJET 720 5424, D/A1, Mono          |CCP000 182.0 23.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x028D
Plotter009=*TechJET 720 5436, E/A0, Mono          |CCP000 182.0 35.00  360.0  360.0 0x0919 255 94 0 3 9600 2 7 1 0 0x028D

[ CalComp Solus 4 LED Plotters         ADI 4.2 V6.50 - by CalComp]
NumPlotters=2
Plotter000=*Solus 4 LED  54436, E/A0              |CCP000 96.00 35.75  400.0  400.0 0x0119 255 16 0 3 9600 2 7 1 0 0x035D
Plotter001=*Solus 4 LED  54436, E/A0              |CCP000 96.00 35.75  400.0  400.0 0x0119 255 16 0 3 9600 2 7 1 0 0x035D
Plotter002=*Solus 4 LED  54424, D/A1              |CCP000 72.00 23.50  400.0  400.0 0x0119 255 16 0 3 9600 2 7 1 0 0x035D

[ CalComp DrawingMaster Plotters       ADI 4.2 V6.50 - by CalComp]
NumPlotters=6
Plotter000=*DrawingMaster 800 53436, E/A0         |CCP000 161.4 35.20  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x033D
Plotter001=*DrawingMaster 800 53436, E/A0         |CCP000 161.4 35.20  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x033D
Plotter002=*DrawingMaster 600 53336, E/A0         |CCP000 161.4 35.20  300.0  300.0 0x0919 255 16 0 3 9600 2 7 1 0 0x033D
Plotter003= DrawingMaster Plus 52436, E/A0        |CCP000 161.4 35.20  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x023D
Plotter004=*DrawingMaster Plus 52424, D/A1        |CCP000 161.4 23.58  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x023D
Plotter005=*DrawingMaster Plus 52224, D/A1        |CCP000 327.6 23.58  200.0  200.0 0x0919 255 16 0 3 9600 2 7 1 0 0x023D
Plotter006=*DrawingMaster Plus 52236, E/A0        |CCP000 327.6 35.20  200.0  200.0 0x0919 255 16 0 3 9600 2 7 1 0 0x023D

[ CalComp Electrostatic Plotters       ADI 4.2 V6.50 - by CalComp]
NumPlotters=9
Plotter000= 68444, 44\"  Roll, Color EPP          |CCP000 163.8 43.04  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x031F
Plotter001= 68444, 44\"  Roll, Color EPP          |CCP000 163.8 43.04  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x031F
Plotter002=*68436, E/A0 Roll, Color EPP           |CCP000 163.8 34.76  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x031F
Plotter003=*58444, 44\"  Roll, Color EPP          |CCP000 163.8 43.00  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x0213
Plotter004=*58436, E/A0 Roll, Color EPP           |CCP000 163.8 34.70  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x0213
Plotter005=*58424, D/A1 Roll, Color EPP           |CCP000 163.8 23.00  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x0213
Plotter006=*67436, E/A0 Roll, Monochrome          |CCP000 163.8 35.20  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x031D
Plotter007=*57444, 44\"  Roll, Monochrome         |CCP000 163.8 43.50  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x0211
Plotter008=*57436, E/A0 Roll, Monochrome          |CCP000 163.8 35.20  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x0211
Plotter009=*57424, D/A1 Roll, Monochrome          |CCP000 163.8 23.00  400.0  400.0 0x0919 255 16 0 3 9600 2 7 1 0 0x0211

[ CalComp Pen Plotters                 ADI 4.2 V6.50 - by CalComp]
NumPlotters=11
Plotter000=*DesignMate 3036 E/A0 Sheet            |CCP000 47.50 35.00 1016.0 1016.0 0x1001   8 0 0 3 9600 2 7 1 0 0x0088
Plotter001=*DesignMate 3036 E/A0 Sheet            |CCP000 47.50 35.00 1016.0 1016.0 0x1001   8 0 0 3 9600 2 7 1 0 0x0088
Plotter002=*DesignMate 3024 D/A1 Sheet            |CCP000 34.50 24.70 1016.0 1016.0 0x1001   8 0 0 3 9600 2 7 1 0 0x0088
Plotter003=*Pacesetter Classic 4036 Dual          |CCP000 64.50 35.60 1016.0 1016.0 0x1801   8 0 0 3 9600 2 7 1 0 0x0088
Plotter004= Pacesetter 2036, E/A0 Sheet           |CCP000 45.50 35.60 1016.0 1016.0 0x1001   8 0 0 3 9600 2 7 1 0 0x0088
Plotter005=*Pacesetter 2024, D/A1 Sheet           |CCP000 34.50 24.70 1016.0 1016.0 0x1001   8 0 0 3 9600 2 7 1 0 0x0088
Plotter006= Artisan 1023, D/A1 Sheet              |CCP000 34.50 24.00 1016.0 1016.0 0x1001   8 0 0 1 9600 2 7 1 0 0x0000
Plotter007=*Artisan 1025, E/A0 Sheet              |CCP000 47.50 34.80 1016.0 1016.0 0x1001   8 0 0 1 9600 2 7 1 0 0x0000
Plotter008=*Artisan 1026, E/A0 Dual               |CCP000 64.50 34.80 1016.0 1016.0 0x1801   8 0 0 1 9600 2 7 1 0 0x0000
Plotter009=*1077, E/A0 Dual                       |CCP000 64.50 34.00 1016.0 1016.0 0x1801   4 0 0 1 9600 2 7 1 0 0x0080
Plotter010= 1044, E/A0 Dual Mode                  |CCP000 64.50 34.00 1016.0 1016.0 0x1801   8 0 0 1 9600 2 7 1 0 0x0080
Plotter011= 1043, E/A0 Sheet                      |CCP000 47.40 34.00 1016.0 1016.0 0x1001   8 0 0 1 9600 2 7 1 0 0x0080

;; Model Dependent Options and Defaults
