       +------------------------------------------------------+
       |    ICD-3600AT DOS Driver Version 1.0 Information     |
       +------------------------------------------------------+

This document describes the installation procedure of ICD-3600AT
DOS Driver. Before using the unit, be sure to read this information
with the User's guide.
This driver can be used for DOS and Windows 3.1 only.

If you are going to use ICD-3600AT under Windows 95, Windows NT and
OS/2, you can use the generic drivers attached to the OS.

A. DOS Driver installation - Installation software

    1.Turn on your PC and wait for DOS prompt.
    2.Insert the Option Diskette packaged with the unit into drive A.
    3.Key in A:INSTALL and then execute.
    4.Follow the instructions on the screen.

    Note : This installer (INSTALL.EXE) changes CONFIG.SYS and
           AUTOEXEC.BAT as follows and registers a device driver
           (IDE24CD.SYS) automatically. If you do want to change
           your CONFIG.SYS and AUTOEXEC.BAT by yourself, please
           follow Instruction 'B' (Manual Installation).

           (CONFIG.SYS)
            DEVICE=C:\IDE24CD.SYS /D:ICD3600

           (AUTOEXEC.BAT)
            C:\MSCDEX.EXE /D:ICD3600


B. DOS Driver installation - Manual installation

    1.Turn on your PC and wait for DOS prompt.
    2.Insert the Option Diskette packaged with the unit into drive A.
    3.Copy IDE24CD.SYS from drive A onto your hard disk (C:).  
    4.Check what directory MSCDEX.EXE exists in.
    5.Add the following lines in CONFIG.SYS and AUTOEXEC.BAT by
      using an editor.

           (CONFIG.SYS)
            DEVICE=C:\xxx\IDE24CD.SYS /D:ICD3600
              Herein, xxx is name of the directory where IDE24CD.SYS
              exists.

           (AUTOEXEC.BAT)
            C:\yyy\MSCDEX.EXE /D:ICD3600
              Herein, yyy is name of the directory where MSCDEX.EXE
              exists.

      Note: The device name /D:ICD3600 in CONFIG.SYS and AUTOEXEC.BAT
            can be changed to preferred name, but must be common to
            both files.

    6. After re-booting your system, you can use ICD-3600AT.


C. Driver installation for Windows 3.1

   You can use the DOS driver (IDE24CD.SYS) under Windows 3.1.
   Please follow the instructions described above.
   During installation, be sure that you are under real DOS,
   not DOS window of Windows 3.1.


Windows 3.1, Windows 95 and Windows NT are the trademark of
Microsoft Corporation.
OS/2 is the trademark of IBM Corporation.