Encoder g726 [G.726 ADPCM]:
    General capabilities: small 
    Threading capabilities: none
    Supported sample formats: s16
g726 AVOptions:
  -code_size         <int>        E...A.... Bits per code (from 2 to 5) (default 4)


