Filter vaguedenoiser
  Apply a Wavelet based Denoiser.
    Inputs:
       #0: default (video)
    Outputs:
       #0: default (video)
vaguedenoiser AVOptions:
  threshold         <float>      ..FV..... set filtering strength (from 0 to DBL_MAX) (default 2)
  method            <int>        ..FV..... set filtering method (from 0 to 2) (default garrote)
     hard            0            ..FV..... hard thresholding
     soft            1            ..FV..... soft thresholding
     garrote         2            ..FV..... garotte thresholding
  nsteps            <int>        ..FV..... set number of steps (from 1 to 32) (default 6)
  percent           <float>      ..FV..... set percent of full denoising (from 0 to 100) (default 85)
  planes            <int>        ..FV..... set planes to filter (from 0 to 15) (default 15)

This filter has support for timeline through the 'enable' option.

